{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":60,"n_cols":8,"rows_kept":60,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERSQ-AV1"]
[]
[]
[]
[]
["","","","","","ERSQ011AAV1","ERSQ014AAV1","ERSQ016AAV1"]
["Hladina akustického tlaku","Vytápění","","Jm.","dBA","","53"]
["Standardní příslušenství","Příručka pro instalaci","","","","","1"]
["Chladivo","Vliv na globální oteplování (GWP)","","","","","2,087.5"]
["","Náplň","","","kg","","4.5"]
["","Typ","","","","","R-410A"]
["Provozní rozsah","Vytápění","","Max.","° CWB","","20"]
["","","","Min.","° CWB","","-20"]
["","Teplá užitková voda","","Min.","°CST","","-20"]
["","","","Max.","°CST","","35"]
["Spoje potrubí","Tepelná izolace","","","","","Potrubí kapaliny a plynu"]
["","Kapalina","","Vnější průměr","mm","","9.52"]
["","Plyn","","Vnější průměr","mm","","15.9"]
["","Vypouštění","","OD","mm","","26x3"]
["","Rozdíl hladin","IU - OU","Max.","m","","30"]
["Sound power level","Heating","","Jm.","dBA","","69"]
["Rozměry","Jednotka","","Šířka","mm","","900"]
["","","","Hloubka","mm","","320"]
["","","","Výška","mm","","1,345"]
["Hmotnost","Jednotka","","","kg","","120"]
["Power supply","Fáze","","","","","1~"]
["","Označení","","","","","V1"]
["","Frekvence","","","Hz","","50"]
["","Napětí","","","V","","220-440"]
["Proud","Doporučené jištění","","","A","","25"]
["Poznámky","","","","","","(1) - Viz samostatný výkres s provozním rozsahem"]
["","","","","","","(2) - Zmax: V souladu s EN/IEC 61000-3-11 může být nutné se poradit s distributorem energie a zajistit, aby zařízení bylo připojeno k příkonu s hodnotou Zsys (impedance systému) ≤ Zmax."]
["","","","","","","(3) - EN/IEC 61000-3-11: Europæisk/international teknisk standard, der sætter grænserne for spændingsændringer, spændingssvingninger og flimmer i offentlige lavsspændingsforsyningssystemer for udstyr med mærkestrøm ≤ 75A."]
["","","","","","","(4) - Min. hodnota zkratovaného proudu Ssc: Zařízení je v souladu s normou EN/IEC 61000-3-12: Evropská/mezinárodní norma stanovující standardní nastavení limitů pro harmonický proud vytvářený zařízením připojeným do veřejné sítě nízkého napětí se vstupním proudem > 16 A a ≤ 75 A v každé fázi"]
["","","","","","","(5) - Obsahuje fluorované skleníkové plyny"]
["Rozměry","Jednotka","","Výška","mm","1345","","1345"]
["","","","Šířka","mm","900","","900"]
["","","","Hloubka","mm","320","","320"]
["Hmotnost","Jednotka","","","kg","120","","120"]
["Provozní rozsah","Vytápění","","Min.","° CWB","-20","","-20"]
["","","","Max.","° CWB","20","","20"]
["","Teplá užitková voda","","Min.","°CST","-20","","-20"]
["","","","Max.","°CST","35","","35"]
["Hladina akustického výkonu","Vytápění","","Jm.","dBA","68","","71"]
["Hladina akustického tlaku","Vytápění","","Jm.","dBA","52","","55"]
["Chladivo","Typ","","","","R-410A","","R-410A"]
["","Vliv na globální oteplování (GWP)","","","","2087.5","","2087.5"]
["","Náplň","","","tCO2Eq","9.4","","9.4"]
["","Náplň","","","kg","4.5","","4.5"]
["Připojovací rozměry","Kapalina","","Vnější průměr","mm","9.52","","9.52"]
["","Plyn","","Vnější průměr","mm","15.9","","15.9"]
["Spoje potrubí","Vypouštění","","OD","mm","26x3","","26x3"]
["","Rozdíl hladin","IU - OU","Max.","m","30","","30"]
["Připojovací rozměry","Tepelná izolace","","","","Potrubí kapaliny a plynu","","Potrubí kapaliny a plynu"]
["Standardní příslušenství","Installation manual","","","","1","","1"]
["Napájení","Označení","","","","V1","","V1"]
["","Fáze","","","","1~","","1~"]
["","Frekvence","","","Hz","50","","50"]
["","Napětí","","","V","220-440","","220-440"]
["Proud","Doporučené jištění","","","A","25","","25"]