{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":8,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETBX16E9W / EPRA014-018DW"]
[]
[]
[]
[]
["","","","","","ETBX16EF9W / EPRA14DAW1","ETBX16EF9W / EPRA16DAW1","ETBX16EF9W / EPRA18DAW1"]
["COP","","","","","4.79","5.00 (2)","5.00"]
["Prostorové vytápění","Výstup vody 55 °C v průměrném podnebí","Obecně","Třída celoroční účinnosti prostorového vytápění","","","A++"]
["","","","ηs (Celoroční účinnost prostorového vytápění)","%","","142"]
["","","","SCOP","","","3.63"]
["Chladicí výkon","Jm.","","","kW","","11.5 (3), 7.88 (4)"]
["EER","","","","","4.13, 2.70","4.11 (3), 2.69 (4)","4.09, 2.68"]
["Topný výkon","Jm.","","","kW","","9.00 (2)"]
["","Min.","","","kW","","3.96 (1)"]
["","Max.","","","kW","","10.44 (1)"]
["Vstup napájení","Chlazení","","Jm.","kW","","2.80 (3), 2.93 (4)"]
["","Vytápění","","Max.","kW","","2.32 (5)"]
["","","","Min.","kW","","0.90 (5)"]
["","","","Jm.","kW","","1.80 (2)"]
["Poznámky","","","","","(1) - Výkon podle normy EN14511 a platné pro teplotu vody v rozsahu dT = 3~8 °C při Ta 7 °C","(1) - Výkon podle normy EN14511 a platné pro teplotu vody v rozsahu dT = 3~8 °C při Ta 7 °C","(1) - Výkon podle normy EN14511 a platné pro teplotu vody v rozsahu dT = 3~8 °C při Ta 7 °C"]
["","","","","","(2) - Betingelse: Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(2) - Betingelse: Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(2) - Betingelse: Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","","(3) - Chlazení: EW 23 °C; LW 18 °C; podmínky okolního prostředí: 35 °CDB","(3) - Chlazení: EW 23 °C; LW 18 °C; podmínky okolního prostředí: 35 °CDB","(3) - Chlazení: EW 23 °C; LW 18 °C; podmínky okolního prostředí: 35 °CDB"]
["","","","","","(4) - Chlazení: EW 12 °C; LW 7 °C; podmínky okolního prostředí: 35 °CDB","(4) - Chlazení: EW 12 °C; LW 7 °C; podmínky okolního prostředí: 35 °CDB","(4) - Chlazení: EW 12 °C; LW 7 °C; podmínky okolního prostředí: 35 °CDB"]
["","","","","","(5) - Příkon je celkový příkon vnitřních a venkovních jednotek, včetně cirkulačního čerpadla; podle normy EN14511","(5) - Příkon je celkový příkon vnitřních a venkovních jednotek, včetně cirkulačního čerpadla; podle normy EN14511","(5) - Příkon je celkový příkon vnitřních a venkovních jednotek, včetně cirkulačního čerpadla; podle normy EN14511"]
["","","","","","(6) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) při plném výkonu čerpadla","(6) - Test při Ta ST/MT 7 °C/6 °C. Dle EN 16147.","(6) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) při plném výkonu čerpadla"]
["","","","","","","(7) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) při plném výkonu čerpadla"]
["Topný výkon","Min.","","","kW","3.70","","4.40"]
["","Jm.","","","kW","5.90","","9.00"]
["","Max.","","","kW","9.75","","11.60"]
["Chladicí výkon","Jm.","","","kW","10.6, 6.90","","12.5, 8.86"]
["Vstup napájení","Vytápění","","Min.","kW","0.84","","1.00"]
["","","","Jm.","kW","1.23","","1.80"]
["","","","Max.","kW","2.17","","2.58"]
["","Chlazení","","Jm.","kW","2.55, 2.56","","3.05, 3.31"]
["Prostorové vytápění","Prostorové vytápění-=-Výstup vody 55&nbsp;°C v&nbsp;průměrném podnebí","Prostorové vytápění-=-Výstup vody 55&nbsp;°C v&nbsp;průměrném podnebí-=-Obecné","Prostorové vytápění-=-Výstup vody 55&nbsp;°C v&nbsp;průměrném podnebí-=-Obecné-=-SCOP","","3.63","","3.63"]
["","","Prostorové vytápění-=-Výstup vody 55&nbsp;°C v&nbsp;průměrném podnebí-=-Obecně","Prostorové vytápění-=-Výstup vody 55&nbsp;°C v&nbsp;průměrném podnebí-=-Obecně-=-Třída celoroční účinnosti prostorového vytápění","","A++","","A++"]
["","Prostorové vytápění-=-Výstup vody 35°C v&nbsp;průměrném podnebí","Prostorové vytápění-=-Výstup vody 35°C v&nbsp;průměrném podnebí-=-Obecné","Prostorové vytápění-=-Výstup vody 35°C v&nbsp;průměrném podnebí-=-Obecné-=-SCOP","","4.81","","4.81"]
["","","","Prostorové vytápění-=-Výstup vody 35°C v&nbsp;průměrném podnebí-=-Obecné-=-Třída celoroční účinnosti prostorového vytápění","","A+++","","A+++"]