{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":11,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSHB12E / EPRA08-12EW"]
[]
[]
[]
[]
["","","","","","ETSHB12P30EF / EPRA08EAW1","ETSHB12P50EF / EPRA08EAW1","ETSHB12P30EF / EPRA10EAW1","ETSHB12P50EF / EPRA10EAW1","ETSHB12P30EF / EPRA12EAW1","ETSHB12P50EF / EPRA12EAW1"]
["Vnitřní jednotka","","","","","ETSHB12P30EF","ETSHB12P50EF","ETSHB12P30EF","ETSHB12P50EF","ETSHB12P30EF","ETSHB12P50EF"]
["Topný výkon","Jm.","","","kW","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)"]
["Vstup napájení","Vytápění","","Jm.","kW","1.21 (1)","1.21 (1)","1.21 (1)","1.21 (1)","1.21 (1)","1.21 (1)"]
["COP","","","","","5.1","5.1","5.1","5.1","5.1","5.1"]
["Ohřev užitkové vody","Obecně","","Deklarovaný profil zátěže","","L","XL","L","XL","L","XL"]
["","Průměrné podnebí","","Třída energetické účinnosti ohřevu vody","","A+","A+","A+","A+","A+","A+"]
["Prostorové vytápění","Prostorové vytápění-=-Výstup vody 55&nbsp;°C v&nbsp;průměrném podnebí","Prostorové vytápění-=-Výstup vody 55&nbsp;°C v&nbsp;průměrném podnebí-=-Obecné","Prostorové vytápění-=-Výstup vody 55&nbsp;°C v&nbsp;průměrném podnebí-=-Obecné-=-SCOP","","3.52","3.52","3.53","3.53","3.53","3.53"]
["","","Prostorové vytápění-=-Výstup vody 55&nbsp;°C v&nbsp;průměrném podnebí-=-Obecně","Prostorové vytápění-=-Výstup vody 55&nbsp;°C v&nbsp;průměrném podnebí-=-Obecně-=-Třída celoroční účinnosti prostorového vytápění","","A++","A++","A++","A++","A++","A++"]
["","Prostorové vytápění-=-Výstup vody 35°C v&nbsp;průměrném podnebí","Prostorové vytápění-=-Výstup vody 35°C v&nbsp;průměrném podnebí-=-Obecné","Prostorové vytápění-=-Výstup vody 35°C v&nbsp;průměrném podnebí-=-Obecné-=-SCOP","","4.81","4.81","4.84","4.84","4.84","4.84"]
["","","","Prostorové vytápění-=-Výstup vody 35°C v&nbsp;průměrném podnebí-=-Obecné-=-Třída celoroční účinnosti prostorového vytápění","","A+++","A+++","A+++","A+++","A+++","A+++"]
["Poznámky","","","","","(1) - Podmínky 1: chlazení Ta 35°C - LWE 18℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Podmínky 1: chlazení Ta 35°C - LWE 18℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Podmínky 1: chlazení Ta 35°C - LWE 18℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Podmínky 1: chlazení Ta 35°C - LWE 18℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Podmínky 1: chlazení Ta 35°C - LWE 18℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Podmínky 1: chlazení Ta 35°C - LWE 18℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","","(2) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) při plném výkonu čerpadla","(2) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) při plném výkonu čerpadla","(2) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) při plném výkonu čerpadla","(2) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) při plném výkonu čerpadla","(2) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) při plném výkonu čerpadla","(2) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) při plném výkonu čerpadla"]