{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B / ARXM-R"]
[]
[]
[]
[]
["","","","","FAA71BUV1B / ARXM71R2V1B","FAA71BUV1B / ARXM71R5V1B"]
["Chladicí výkon","Jm.","","kW","6.80","6.80"]
["","Max.","","kW","6.95","6.95"]
["Topný výkon","Jm.","","kW","7.50","7.50"]
["","Max.","","kW","7.59","7.59"]
["Jmenovitá účinnost","EER","","","3.40","3.40"]
["","COP","","","3.19","3.19"]
["","Roční spotřeba energie","","kWh","1000","1000"]
["","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích-=-Chlazení","","A","A"]
["","","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích-=-Vytápění","","D","D"]
["Prostorové chlazení","Třída energetické úspornosti","","","A+","A+"]
["","Kapacita","Pnávrh","kW","6.80","6.80"]
["","SEER","","","5.77","5.77"]
["","Roční spotřeba energie","","kWh/r","412","412"]
["Prostorové vytápění (průměrné klima)","Třída energetické účinnosti","","","A","A"]
["","Výkon","Pnávrh","kW","4.50","4.50"]
["","SCOP/A","","","3.81","3.81"]
["","Topný výkon Pdh při -10°","","kW","4.50","4.50"]
["","Roční spotřeba energie","","kWh/r","1652","1652"]
["Energetickou účinná řada","","","","A+++ ~ D","A+++ ~ D"]