{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":6,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B / RZASG-MY"]
[]
[]
[]
[]
["","","","","FAA100BUV1B / RZASG100MUY","FAA71BUV1B / FAA71BUV1B / RZASG140MUY"]
["Chladicí výkon","Jm.","","kW","9.5","13.4 (1)"]
["Topný výkon","Jm.","","kW","10.8 (2)","15.5 (2)"]
["Prostorové chlazení","Třída energetické úspornosti","","","A+"]
["","Kapacita","Pnávrh","kW","9.5","13.4"]
["","SEER","","","5.83","8.15"]
["","Roční spotřeba energie","","kWh/rok","570","986"]
["Prostorové vytápění (průměrné klima)","Třída energetické účinnosti","","","A"]
["","Výkon","Pnávrh","kW","6","7.8"]
["","SCOP/A","","","3.85","4.53"]
["","Roční spotřeba energie","","kWh/rok","2182","2409"]
["Poznámky","","","","(1) - Jmenovité chladicí výkony vycházejí z těchto podmínek: vnitřní tep.: 27°CDB, 19°CWB, venkovní teplota: 35 °CDB, ekvivalentní délka potrubí s chladivem: 5 m, rozdíl úrovní: 0 m.","(1) - Jmenovité chladicí výkony vycházejí z těchto podmínek: vnitřní tep.: 27°CDB, 19°CWB, venkovní teplota: 35 °CDB, ekvivalentní délka potrubí s chladivem: 5 m, rozdíl úrovní: 0 m."]
["","","","","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m.","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m."]