{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":9,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAQ-C9 / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FAQ100CVEB9 / RZQG71L9V1B","FAQ71CVEB9 / RZQG71L9V1B","FAQ100CVEB9 / RZQG100L9V1B","FAQ71CVEB9 / FAQ71CVEB9 / RZQG100L9V1B","FAQ71CVEB9 / FAQ71CVEB9 / RZQG125L9V1B"]
["Chladicí výkon","Jm.","","kW","","6.8","9.5"]
["Prostorové chlazení","SEER","","","6.51","6.43","6.11","5.10","5.10"]
["","Roční spotřeba energie","","kWh/a","366","371","545","652","824"]
["","Kapacita","Pnávrh","kW","6.80","6.80","9.50","9.50","12.00"]
["","Třída energetické úspornosti","","","A++","A++","A++","B","B"]
["Prostorové vytápění (průměrné klima)","Výkon","Pnávrh","kW","6.33","6.33","10.20","11.30","12.71"]
["","SCOP/A","","","4.02","4.02","4.01","3.80","3.80"]
["","Třída energetické účinnosti","","","A+","A+","A+","A","A"]
["","Roční spotřeba energie","","kWh/a","2,205","2,205","3,562","4,164","4,683"]
["Jmenovitá účinnost","Roční spotřeba energie","","kWh","","1,000","1,315"]
["","EER","","","","3.40","3.62"]
["","COP","","","","3.70","3.61"]
["","Směrnice o energetických štítcích","Chlazení","","","A","A"]
["","","Vytápění","","","A","A"]
["Topný výkon","Jm.","","kW","","7.5","10.8"]
["Poznámky","","","","","(1) - Roční spotřeba energie odpovídá Směrnici 2002/31/ES o uvádění spotřeby energie na energetických štítcích klimatizátorů vzduchu pro domácnost","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU"]
["","","","","","(2) - SEER a SCOP odpovídají EN 14825","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení"]
["","","","","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","","","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU"]