{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAQ-C9"]
[]
[]
[]
[]
["","","","","FAQ71CVEB9","FAQ100CVEB9"]
["Hladina akustického tlaku","Vytápění","Vysoké","dBA","45","49"]
["","","Jm.","dBA","42","45"]
["","","Střední","dBA","42","45"]
["","","Nízký","dBA","40","41"]
["","Chlazení","Střední","dBA","42","45"]
["","","Nízký","dBA","40","41"]
["","","Vysoké","dBA","45","49"]
["","","Jm.","dBA","42","45"]
["Chladicí výkon","Total capacity","Jm.","kW","0.051","0.061"]
["Spoje potrubí","Liquid","OD","mm","9.52","9.52"]
["","Plyn","OD","mm","15.9","15.9"]
["","Vypouštění","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["Hladina akustického výkonu","Chlazení","","dBA","61","65"]
["","Vytápění","","dBA","61","65"]
["Rozměry","Jednotka","Šířka","mm","1,050","1,200"]
["","","Hloubka","mm","238","240"]
["","","Výška","mm","290","340"]
["Casing","Material","","","Pryskyřice","Pryskyřice"]
["","Barva","","","Čerstvý bílý","Čerstvý bílý"]
["Hmotnost","Jednotka","","kg","13","17"]
["Topný výkon","Total capacity","Jmen.","kW","0.068","0.061"]
["Power supply","Fáze","","","1~","1~"]
["","Frekvence","","Hz","50","50"]
["","Napětí","","V","220-240","220-240"]