{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / RZQ-C"]
[]
[]
[]
[]
["","","","","FBA50A2VEB9 / FBA50A2VEB9 / FBA50A2VEB9 / FBA50A2VEB9 / RZQ200C7Y1B","FBA60A2VEB9 / FBA60A2VEB9 / FBA60A2VEB9 / FBA60A2VEB9 / RZQ250C7Y1B"]
["Chladicí výkon","Jm.","","kW","20.0 (1)"]
["Prostorové chlazení","SEER","","","5.67"]
["","Roční spotřeba energie","","kWh/a","2,115"]
["","Kapacita","Pnávrh","kW","20.0"]
["Prostorové vytápění (průměrné klima)","Výkon","Pnávrh","kW","11.2"]
["","SCOP/A","","","3.68"]
["","Roční spotřeba energie","","kWh/a","4,257"]
["Topný výkon","Jm.","","kW","23.0 (2)"]
["Poznámky","","","","(1) - Chlazení: vnitřní teplota 27° CDB, 19° CWB; vnější teplota 35 °CST; ekvivalentní délka potrubí: 7,5 m; rozdíl úrovně: 0m","(1) - Chlazení: vnitřní teplota 27° CDB, 19° CWB; vnější teplota 35 °CST; ekvivalentní délka potrubí: 7,5 m; rozdíl úrovně: 0m"]
["","","","","(2) - Vytápění: vnitřní teplota 20° CDB; vnější teplota 7° CDB, 6° CWB ekvivalentní délka potrubí chladiva: 7,5 m; rozdíl úrovně: 0m","(2) - Vytápění: vnitřní teplota 20° CDB; vnější teplota 7° CDB, 6° CWB ekvivalentní délka potrubí chladiva: 7,5 m; rozdíl úrovně: 0m"]
["","","","","(3) - Tato hodnota nezahrnuje snížení výkonu při rozmrazování.","(3) - Tato hodnota nezahrnuje snížení výkonu při rozmrazování."]
["Chladicí výkon","Jm.","","kW","","24.1 (1)"]
["Topný výkon","Jm.","","kW","","26.4 (2)"]
["Prostorové chlazení","Kapacita","Pnávrh","kW","","24.1"]
["","SEER","","","","5.74"]
["","Roční spotřeba energie","","kWh/a","","2518"]
["Prostorové vytápění (průměrné klima)","Výkon","Pnávrh","kW","","12.1"]
["","SCOP/A","","","","3.76"]
["","Roční spotřeba energie","","kWh/a","","4484"]
["Energetickou účinná řada","","","","","A+++ ~ D"]