{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A / 4MXM-N"]
[]
[]
[]
[]
["","","","","FBA35A2VEB / FBA35A2VEB / 4MXM68N2V1B"]
["Chladicí výkon","Jm.","","kW","6.8"]
["Prostorové chlazení","SEER","","","5.26"]
["","Roční spotřeba energie","","kWh/a","453"]
["","Kapacita","Pnávrh","kW","6.80"]
["","Třída energetické úspornosti","","","A"]
["Prostorové vytápění (průměrné klima)","Výkon","Pnávrh","kW","3.60"]
["","SCOP/A","","","3.81"]
["","Třída energetické účinnosti","","","A"]
["","Roční spotřeba energie","","kWh/a","1,323"]
["Jmenovitá účinnost","Roční spotřeba energie","","kWh","1,245"]
["","EER","","","2.73"]
["","COP","","","3.24"]
["","Směrnice oenergetických štítcích","Chlazení","","D"]
["","","Vytápění","","C"]
["Topný výkon","Jm.","","kW","8.60"]
["Poznámky","","","","(1) - Údaje o elektrickém systému najdete v samostatném výkresu"]