{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A / RXM-N"]
[]
[]
[]
[]
["","","","","FBA50A2VEB / RXM50N2V1B","FBA60A2VEB / RXM60N2V1B"]
["Chladicí výkon","Jm.","","kW","5.00","5.70"]
["Prostorové chlazení","Roční spotřeba energie","","kWh/r","","337"]
["","Kapacita","Pnávrh","kW","","5.70"]
["Prostorové vytápění (průměrné klima)","Výkon","Pnávrh","kW","","4.60"]
["","Roční spotřeba energie","","kWh/r","","1,607"]
["Jmenovitá účinnost","Annual energy consumption","","kWh","704","818"]
["","EER","","","3.55","3.48"]
["","COP","","","3.83","3.71"]
["","Směrnice o energetických štítcích","Chlazení","","A","A"]
["","","Vytápění","","A","A"]
["Topný výkon","Jm.","","kW","5.50","7.00"]
["Poznámky","","","","(1) - Viz samostatný výkres s provozním rozsahem","(1) - Viz samostatný výkres s provozním rozsahem"]
["","","","","(2) - Údaje o elektrickém systému najdete v samostatném výkresu","(2) - Údaje o elektrickém systému najdete v samostatném výkresu"]
["","","","","(3) - Jmenovité chladicí výkony vycházejí z těchto podmínek: vnitřní teplota: 27°CDB, 19°CWB, venkovní teplota: 35 °CDB, ekvivalentní délka potrubí s chladivem: 5 m, rozdíl úrovní: 0 m.","(3) - Jmenovité chladicí výkony vycházejí z těchto podmínek: vnitřní tep.: 27°CDB, 19°CWB, venkovní teplota: 35 °CDB, ekvivalentní délka potrubí s chladivem: 5 m, rozdíl úrovní: 0 m."]
["","","","","(4) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m.","(4) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m."]
["Prostorové chlazení","Třída energetické úspornosti","","","","A+"]
["","SEER","","","","5.91"]
["Prostorové vytápění (průměrné klima)","Třída energetické účinnosti","","","","A+"]
["","SCOP/A","","","","4.01"]