{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":12,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-C8 / RZQSG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FBQ100C8VEB / RZQSG100L8Y1B","FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / RZQSG100L8Y1B","FBQ50C8VEB / FBQ50C8VEB / RZQSG100L8Y1B","FBQ125C8VEB / RZQSG125L8Y1B","FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / RZQSG125L8Y1B","FBQ50C8VEB / FBQ50C8VEB / FBQ50C8VEB / RZQSG125L8Y1B","FBQ60C8VEB / FBQ60C8VEB / RZQSG125L8Y1B","FBQ140C8VEB / RZQSG140L7Y1B"]
["Chladicí výkon","Jm.","","kW","9.5","","","12.0","","","","13.4"]
["Prostorové chlazení","SEER","","","5.5","5.1","5.1","5.2","4.8","4.8","4.8"]
["","Roční spotřeba energie","","kWh/rok","605","652","652","808","875","875","875"]
["","Kapacita","Pnávrh","kW","9.5","9.5","9.5","12","12","12","12"]
["","Třída energetické úspornosti","","","A","B","B","A","B","B","B"]
["Prostorové vytápění (průměrné klima)","Výkon","Pnávrh","kW","7.6","7.6","7.6","7.6","7.6","7.6","7.6"]
["","SCOP/A","","","4.01","3.8","3.8","3.9","3.8","3.8","3.8"]
["","Třída energetické účinnosti","","","A+","A","A","A","A","A","A"]
["","Roční spotřeba energie","","kWh/rok","2,654","2,800","2,800","2,729","2,800","2,800","2,800"]
["Jmenovitá účinnost","Roční spotřeba energie","","kWh","1,435","","","1,870","","","","2,220"]
["","EER","","","3.31","","","3.21","","","","3.02"]
["","COP","","","3.65","","","3.51","","","","3.41"]
["","Směrnice oenergetických štítcích","Chlazení","","A","","","A"]
["","","Vytápění","","A","","","B"]
["Topný výkon","Jm.","","kW","10.8","","","13.5","","","","15.5"]
["Poznámky","","","","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","","","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","","","","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU"]
["","","","","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení","","","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení","","","","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení"]
["","","","","","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU"]