{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-D / RXS-L"]
[]
[]
[]
[]
["","","","","FBQ50D2VEB / RXS50L2V1B","FBQ60D2VEB / RXS60L2V1B (Archived)"]
["Chladicí výkon","Jm.","","kW","5.0 (2)"]
["Jmenovitá účinnost","Roční spotřeba energie","","kWh","710"]
["","EER","","","3.52 (1)"]
["","COP","","","3.83 (1)"]
["","Směrnice oenergetických štítcích","Chlazení","","A"]
["","","Vytápění","","A"]
["Topný výkon","Jm.","","kW","5.50 (2)"]
["Poznámky","","","","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU"]
["","","","","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení"]
["Venkovní jednotka","","","","","RXS60L"]
["Chladicí výkon","Jm.","","kW","","5.7"]
["Topný výkon","Jm.","","kW","","7.00"]
["Jmenovitá účinnost","EER","","","","3.45"]
["","COP","","","","3.71"]
["","Roční spotřeba energie","","kWh","","826"]
["","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích-=-Chlazení","","","A"]
["","","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích-=-Vytápění","","","A"]
["Prostorové chlazení","Třída energetické úspornosti","","","","A+"]
["","Kapacita","Pnávrh","kW","","5.70"]
["","SEER","","","","5.86"]
["","Roční spotřeba energie","","kWh/a","","340"]
["Prostorové vytápění (průměrné klima)","Třída energetické účinnosti","","","","A+"]
["","Výkon","Pnávrh","kW","","4.60"]
["","SCOP/A","","","","4.01"]
["","Roční spotřeba energie","","kWh/a","","1606"]