{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":12,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-D / RZQSG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FBQ100D2VEB / RZQSG100L8Y1B","FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / RZQSG100L8Y1B","FBQ50D2VEB / FBQ50D2VEB / RZQSG100L8Y1B","FBQ125D2VEB / RZQSG125L8Y1B","FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / RZQSG125L8Y1B","FBQ50D2VEB / FBQ50D2VEB / FBQ50D2VEB / RZQSG125L8Y1B","FBQ60D2VEB / FBQ60D2VEB / RZQSG125L8Y1B","FBQ140D2VEB / RZQSG140L7Y1B"]
["Chladicí výkon","Jm.","","kW","9.5 (2)","","","12.0 (2)","","","","13.4 (2)"]
["Prostorové chlazení","SEER","","","5.61","5.10","5.10","5.47","4.80","4.80","4.80"]
["","Roční spotřeba energie","","kWh/r","593","652","652","768","875","875","875"]
["","Kapacita","Pnávrh","kW","9.50","9.50","9.50","12.00","12.00","12.00","12.00"]
["","Třída energetické úspornosti","","","A+","A","A","A","B","B","B"]
["Prostorové vytápění (průměrné klima)","Výkon","Pnávrh","kW","7.60","7.60","7.60","7.60","7.60","7.60","7.60"]
["","SCOP/A","","","4.15","3.80","3.80","4.01","3.80","3.80","3.80"]
["","Třída energetické účinnosti","","","A+","A","A","A+","A","A","A"]
["","Roční spotřeba energie","","kWh/r","2,564","2,800","2,800","2,653","2,800","2,800","2,800"]
["Jmenovitá účinnost","Annual energy consumption","","kWh","1,418","","","1,858"]
["","EER","","","3.35 (1)","","","3.23 (1)","","","","3.06 (1)"]
["","COP","","","3.67 (1)","","","3.63 (1)","","","","3.40 (1)"]
["","Směrnice o energetických štítcích","Chlazení","","A","","","A"]
["","","Vytápění","","A","","","A"]
["Topný výkon","Jm.","","kW","10.80 (2)","","","13.50 (2)","","","","15.50 (2)"]
["Poznámky","","","","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","","","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","","","","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU"]
["","","","","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení","","","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení","","","","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení"]
["","","","","(3) - Roční spotřeba energie odpovídá Směrnici 2002/31/ES o uvádění spotřeby energie na energetických štítcích klimatizátorů vzduchu pro domácnost","","","(3) - Roční spotřeba energie odpovídá Směrnici 2002/31/ES o uvádění spotřeby energie na energetických štítcích klimatizátorů vzduchu pro domácnost"]
["","","","","(4) - SEER a SCOP odpovídají EN 14825","","","(4) - SEER a SCOP odpovídají EN 14825"]
["","","","","","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU"]