{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":8,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / AZAS-MV1"]
[]
[]
[]
[]
["","","","","FCAG100AVEB / AZAS100M7V1B","FCAG71AVEB / AZAS71M2V1B","FCAG125AVEB / AZAS125M7V1B","FCAG140AVEB / AZAS140M7V1B"]
["Chladicí výkon","Jm.","","kW","","6.80 (1)","12.1 (1)","13.4 (1)"]
["Topný výkon","Jm.","","kW","","7.50 (2)","13.5 (2)","15.5 (2)"]
["Prostorové chlazení","Třída energetické úspornosti","","","","A+"]
["","Kapacita","Pnávrh","kW","","6.80","12.1","13.0"]
["","SEER","","","","5.87","5.40","6.00"]
["","Roční spotřeba energie","","kWh/rok","","405","1,345","1,300"]
["Prostorové vytápění (průměrné klima)","Třída energetické účinnosti","","","","A"]
["","Výkon","Pnávrh","kW","","4.50","6.00","7.80"]
["","SCOP/A","","","","4.00","3.80","4.31"]
["","Roční spotřeba energie","","kWh/rok","","1,575","2,211","2,534"]
["Poznámky","","","","","(1) - Chlazení: T2: vnitřní teplota 26,6 °CST, 19,4 °CMT, venkovní teplota 48 °CST [Btu/h/W]","(1) - Køling: indendørs temp: 27 °CDB, 19,0 °CWB; udendørs temp. 35°CDB; tilsvarende rørlængde: 5m, niveauforskel: 0m","(1) - Køling: indendørs temp: 27 °CDB, 19,0 °CWB; udendørs temp. 35°CDB; tilsvarende rørlængde: 5m, niveauforskel: 0m"]
["","","","","","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m.","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m.","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m."]
["Energetickou účinná řada","","","","A+++ ~ D"]