{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":12,"n_cols":6,"rows_kept":12,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / RR-BV3"]
[]
[]
[]
[]
["","","","","FCAG71AVEB / RR71B8V3B","FCAG100AVEB / RR100B8V3B"]
["Chladicí výkon","Jm.","","kW","7.10 (1)","10.0 (1)"]
["Jmenovitá účinnost","EER","","","2.64","2.61"]
["","Roční spotřeba energie","","kWh","1,345","1,915"]
["","Směrnice o energetických štítcích","Chlazení","","D","D"]
["Poznámky","","","","(1) - Køling: indendørs temp: 27 °CDB, 19,0 °CWB; udendørs temp. 35°CDB; tilsvarende rørlængde: 5m, niveauforskel: 0m","(1) - Køling: indendørs temp: 27 °CDB, 19,0 °CWB; udendørs temp. 35°CDB; tilsvarende rørlængde: 5m, niveauforskel: 0m"]
["","","","","(2) - Varme: indendørs temp: 20 °CDB; udendørs temp. 7 °CDB, 6 °CWB; tilsvarende kølemiddelrørlængde: 5m, niveauforskel: 0m","(2) - Varme: indendørs temp: 20 °CDB; udendørs temp. 7 °CDB, 6 °CWB; tilsvarende kølemiddelrørlængde: 5m, niveauforskel: 0m"]