{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":6,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RXM-A9"]
[]
[]
[]
[]
["","","","","FCAG35BVEB / RXM35A5V1B9","FCAG50BVEB / RXM50A5V1B9"]
["Chladicí výkon","Jm.","","kW","3.5","5"]
["Topný výkon","Jm.","","kW","4.2","6"]
["Jmenovitá účinnost","EER","","","3.72","3.58"]
["","COP","","","3.77","3.7"]
["","Roční spotřeba energie","","kWh","470","698"]
["","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích-=-Chlazení","","A","A"]
["","","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích-=-Vytápění","","A","A"]
["Prostorové chlazení","Třída energetické úspornosti","","","A++","A++"]
["","Kapacita","Pnávrh","kW","3.5","5"]
["","SEER","","","6.51","6.54"]
["","Roční spotřeba energie","","kWh/r","188","268"]
["Prostorové vytápění (průměrné klima)","Třída energetické účinnosti","","","A++","A+"]
["","Výkon","Pnávrh","kW","3.32","4.36"]
["","SCOP/A","","","4.98","4.3"]
["","Topný výkon Pdh při -10°","","kW","2.67","3.86"]
["","Roční spotřeba energie","","kWh/r","933","1418"]
["Energetickou účinná řada","","","","A+++ ~ D","A+++ ~ D"]
["Poznámky","","","","(1) - Viz samostatný výkres s provozním rozsahem","(1) - Jmenovité chladicí výkony vycházejí ztěchto podmínek: vnitřní tep.: 27°CDB, 19°CWB, venkovní teplota: 35°CDB, ekvivalentní délka potrubí schladivem: 5m, rozdíl úrovní: 0m."]
["","","","","(2) - Údaje o elektrickém systému najdete v samostatném výkresu","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m."]
["","","","","(3) - Jmenovité chladicí výkony vycházejí ztěchto podmínek: vnitřní tep.: 27°CDB, 19°CWB, venkovní teplota: 35°CDB, ekvivalentní délka potrubí schladivem: 5m, rozdíl úrovní: 0m.","(3) - Viz samostatný výkres s provozním rozsahem"]
["","","","","(4) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m.","(4) - Údaje o elektrickém systému najdete v samostatném výkresu"]