{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":5,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RXS-L3"]
[]
[]
[]
[]
["","","","","FCAG35BVEB / RXS35L3V1B"]
["Chladicí výkon","Jm.","","kW","3.40"]
["Topný výkon","Jm.","","kW","4.20"]
["Jmenovitá účinnost","Roční spotřeba energie","","kWh","455"]
["","COP","","","3.50"]
["","EER","","","3.74"]
["","Směrnice o energetických štítcích","Chlazení","","A"]
["","","Vytápění","","B"]
["Připojovací rozměry","Vypouštění","OD","mm","VP25 (Vnější průměr 32, vnitřní průměr 25)"]
["","Plyn","Vnější průměr","mm","9.50"]
["","Kapalina","Vnější průměr","mm","6.35"]
["Poznámky","","","","(1) - Za normálního provozu: +22 °C / +32 °C"]
["","","","","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m."]
["","","","","(3) - Viz samostatný výkres s provozním rozsahem"]
["","","","","(4) - Údaje o elektrickém systému najdete v samostatném výkresu"]