{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":10,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RZAG-A"]
[]
[]
[]
[]
["","","","","FCAG50BVEB / RZAG35A2V1B","FCAG35BVEB / RZAG35A2V1B","FCAG50BVEB / RZAG50A2V1B","FCAG60BVEB / RZAG50A2V1B","FCAG71BVEB / RZAG60A2V1B","FCAG60BVEB / RZAG60A2V1B"]
["Chladicí výkon","Min.","","kW","1.6","1.6","1.7","1.7","1.7","1.7"]
["","Jm.","","kW","3.5","3.5","5.0","5.0","6.0","6.0"]
["","Max.","","kW","4.5","4.5","6.0","6.0","6.5","6.5"]
["Topný výkon","Min.","","kW","1.40","1.40","1.50","1.50","1.60","1.60"]
["","Jm.","","kW","4.00","4.00","5.80","5.80","7.00","7.00"]
["","Max.","","kW","5.00","5.00","6.00","6.00","7.50","7.50"]
["Jmenovitá účinnost","EER","","","4.57","4.40","3.90","3.98","3.79","3.40"]
["","COP","","","4.41","4.30","3.71","3.75","3.53","3.40"]
["","Roční spotřeba energie","","kWh","383","398","641","628","792","882"]
["","Směrnice o energetických štítcích","Chlazení","","A","A","A","A","A","A"]
["","","Vytápění","","A","A","A","A","B","C"]
["Prostorové chlazení","Třída energetické úspornosti","","","A++","A++","A++","A++","A++","A++"]
["","Kapacita","Pnávrh","kW","3.50","3.50","5.00","5.00","6.00","6.00"]
["","SEER","","","7.40","7.30","6.80","6.93","6.82","6.60"]
["","Roční spotřeba energie","","kWh/a","166","168","257","252","308","318"]
["Prostorové vytápění (průměrné klima)","Třída energetické účinnosti","","","A+","A+","A+","A+","A+","A+"]
["","Výkon","Pnávrh","kW","3.30","3.30","4.30","4.30","4.60","4.60"]
["","SCOP/A","","","4.41","4.30","4.30","4.35","4.39","4.25"]
["","Roční spotřeba energie","","kWh/a","1,048","1,074","1,398","1,384","1,467","1,515"]