{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":60,"n_cols":8,"rows_kept":60,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-F"]
[]
[]
[]
[]
["","","","","FCAHG100FVEB","FCAHG125FVEB","FCAHG140FVEB","FCAHG71FVEB"]
["Hladina akustického tlaku","Vytápění","Vysoké","dBA","44","45","45"]
["","","Střední","dBA","39","40","41"]
["","","Nízký","dBA","33","35","37"]
["","Chlazení","Střední","dBA","39","40","41"]
["","","Nízký","dBA","33","35","37"]
["","","Vysoké","dBA","44","45","45"]
["Standardní příslušenství","Příručka pro montáž a provoz","","","Příručka pro montáž a provoz","Příručka pro montáž a provoz","Příručka pro montáž a provoz","Příručka pro montáž a provoz"]
["","Příručka pro instalaci","","","Příručka pro instalaci","Příručka pro instalaci","Příručka pro instalaci","Příručka pro instalaci"]
["Chladivo","Vliv na globální oteplování (GWP)","","","675","675","675","675"]
["Piping connections","Kapalina","Vnější průměr","mm","9.52","9.52","9.52","9.52"]
["","Plyn","Vnější průměr","mm","15.9","15.9","15.9"]
["","Vypouštění","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)"]
["Dekorační panel 4","Rozměry","Hloubka","mm","950","950","950","950"]
["","","Šířka","mm","950","950","950","950"]
["","","Výška","mm","50","50","50","50"]
["","Model","","","BYCQ140D7W1 – Bílá s šedivými klapkami","BYCQ140D7W1 – Bílá s šedivými klapkami","BYCQ140D7W1 – Bílá s šedivými klapkami","BYCQ140D7W1 – Bílá s šedivými klapkami"]
["","Barva","","","Čistě bílá (RAL 9010)","Čistě bílá (RAL 9010)","Čistě bílá (RAL 9010)","Čistě bílá (RAL 9010)"]
["","Hmotnost","","kg","5.4","5.4","5.4","5.4"]
["Hladina akustického výkonu","Chlazení","","dBA","61","61","61"]
["","Vytápění","","dBA","61","61","61"]
["Rozměry","Jednotka","Šířka","mm","840","840","840","840"]
["","","Hloubka","mm","840","840","840","840"]
["","","Výška","mm","288","288","288","288"]
["Opláštění","Materiál","","","Pozinkovaný ocelový plech","Pozinkovaný ocelový plech","Pozinkovaný ocelový plech","Pozinkovaný ocelový plech"]
["Hmotnost","Jednotka","","kg","26.0","26.0","26.0","25.0"]
["Dekorační panel","Hmotnost","","kg","10","10","10"]
["","Model","","","BYCQ140D7GFW1 – panel s automatickým čištěním s jemnou mřížkou filtru","BYCQ140D7GFW1 – panel s automatickým čištěním s jemnou mřížkou filtru","BYCQ140D7GFW1 – panel s automatickým čištěním s jemnou mřížkou filtru"]
["","Rozměry","Výška","mm","130","130","130"]
["","","Hloubka","mm","950","950","950"]
["","","Šířka","mm","950","950","950"]
["","Barva","","","Čistě bílá (RAL 9010)","Čistě bílá (RAL 9010)","Čistě bílá (RAL 9010)"]
["Power supply","Fáze","","","1~","1~","1~","1~"]
["","Frekvence","","Hz","50/60","50/60","50/60","50/60"]
["","Označení","","","VE","VE","VE","VE"]
["","Napětí","","V","220-240","220-240","220-240","220-240"]
["Poznámky","","","","(1) - BYCQ140D7W1W má bílé izolace. Uvědomte si, že usazování nečistot na bílé izolaci je více viditelné a proto není doporučeno instalovat dekorační panel BYCQ140D7W1W v místech vystavených koncentraci nečistot.","(1) - BYCQ140D7W1W má bílé izolace. Uvědomte si, že usazování nečistot na bílé izolaci je více viditelné a proto není doporučeno instalovat dekorační panel BYCQ140D7W1W v místech vystavených koncentraci nečistot.","(1) - BYCQ140D7W1W má bílé izolace. Uvědomte si, že usazování nečistot na bílé izolaci je více viditelné a proto není doporučeno instalovat dekorační panel BYCQ140D7W1W v místech vystavených koncentraci nečistot.","(1) - BYCQ140D7W1W má bílé izolace. Uvědomte si, že usazování nečistot na bílé izolaci je více viditelné a proto není doporučeno instalovat dekorační panel BYCQ140D7W1W v místech vystavených koncentraci nečistot."]
["","","","","(2) - Obsahuje fluorované skleníkové plyny","(2) - Obsahuje fluorované skleníkové plyny","(2) - Obsahuje fluorované skleníkové plyny","(2) - Obsahuje fluorované skleníkové plyny"]
["","","","","(3) - Lydeffektniveauet er en absolut værdi, som viser den styrke, som en lydkilde frembringer.","(3) - Lydeffektniveauet er en absolut værdi, som viser den styrke, som en lydkilde frembringer.","(3) - Lydeffektniveauet er en absolut værdi, som viser den styrke, som en lydkilde frembringer.","(3) - Lydeffektniveauet er en absolut værdi, som viser den styrke, som en lydkilde frembringer."]
["Hladina akustického tlaku","Vytápění","Vysoké","dBA","","","","36"]
["","","Střední","dBA","","","","33"]
["","","Nízký","dBA","","","","29"]
["","Chlazení","Střední","dBA","","","","33"]
["","","Nízký","dBA","","","","29"]
["","","Vysoké","dBA","","","","36"]
["Piping connections","Plyn","Vnější průměr","mm","","","","15.9"]
["","Vypouštění","","","","","","VP25 (I.D. 25/O.D. 32)"]
["Hladina akustického výkonu","Chlazení","","dBA","","","","53"]
["","Vytápění","","dBA","","","","53"]
["Dekorační panel","Hmotnost","","kg","","","","10"]
["","Model","","","","","","BYCQ140D7GFW1 – panel s automatickým čištěním s jemnou mřížkou filtru"]
["","Rozměry","Výška","mm","","","","130"]
["","","Hloubka","mm","","","","950"]
["","","Šířka","mm","","","","950"]
["","Barva","","","","","","Čistě bílá (RAL 9010)"]