{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":5,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-G / RZAG-NV1"]
[]
[]
[]
[]
["","","","","FCAHG100GVEB / RZAG100N7V1B"]
["Chladicí výkon","Jm.","","kW","9.50 (1)"]
["Topný výkon","Jm.","","kW","10.8 (2)"]
["Prostorové chlazení","Třída energetické úspornosti","","","A++"]
["","Kapacita","Pnávrh","kW","9.50"]
["","SEER","","","7.35"]
["","Roční spotřeba energie","","kWh/rok","452"]
["Prostorové vytápění (průměrné klima)","Třída energetické účinnosti","","","A++"]
["","Výkon","Pnávrh","kW","9.52"]
["","SCOP/A","","","4.81"]
["","Roční spotřeba energie","","kWh/rok","2,771"]
["Poznámky","","","","(1) - Chlazení: T2: vnitřní teplota 26,6 °CST, 19,4 °CMT, venkovní teplota 48 °CST [Btu/h/W]"]
["","","","","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m."]