{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":12,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-G / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAHG100GVEB / RZQG100L8Y1B","FCAHG125GVEB / RZQG125L8Y1B","FCAHG71GVEB / RZQG71L8Y1B","FCAHG71GVEB / FCAHG71GVEB / RZQG100L8Y1B","FCAHG140GVEB / RZQG100L8Y1B","FCAHG71GVEB / FCAHG71GVEB / RZQG125L8Y1B","FCAHG140GVEB / RZQG125L8Y1B","FCAHG140GVEB / RZQG140L7Y1B"]
["Energetickou účinná řada","","","","A+++ ~ D","A+++ ~ D","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Chladicí výkon","Jm.","","kW","","","6.80 (1)","","","","","13.4 (1)"]
["Prostorové chlazení","SEER","","","","","6.91","","","","","6.75"]
["","Roční spotřeba energie","","kWh/a","","","345","","","","","1,191"]
["","Kapacita","Pnávrh","kW","","","6.80","","","","","13.4"]
["","Třída energetické úspornosti","","","","","A++"]
["Prostorové vytápění (průměrné klima)","Výkon","Pnávrh","kW","","","7.60","","","","","11.8"]
["","SCOP/A","","","","","4.54","","","","","4.38"]
["","Třída energetické účinnosti","","","","","A+"]
["","Roční spotřeba energie","","kWh/a","","","2,344","","","","","3,766"]
["Jmenovitá účinnost","Roční spotřeba energie","","kWh","","","830"]
["","EER","","","","","4.09 (3)","","","","","3.18 (3)"]
["","COP","","","","","4.80 (3)","","","","","4.12 (3)"]
["","Směrnice oenergetických štítcích","Chlazení","","","","A"]
["","","Vytápění","","","","A"]
["Topný výkon","Jm.","","kW","","","7.50 (2)","","","","","15.5 (2)"]
["Poznámky","","","","","","(1) - Chlazení: vnitřní teplota 27° CDB, 19° CWB; vnější teplota 35 °CST; ekvivalentní délka potrubí: 7,5 m; rozdíl úrovně: 0m","","","","","(1) - Chlazení: vnitřní teplota 27° CDB, 19° CWB; vnější teplota 35 °CST; ekvivalentní délka potrubí: 7,5 m; rozdíl úrovně: 0m"]
["","","","","","","(2) - Vytápění: vnitřní teplota 20° CDB; vnější teplota 7° CDB, 6° CWB ekvivalentní délka potrubí chladiva: 7,5 m; rozdíl úrovně: 0m","","","","","(2) - Vytápění: vnitřní teplota 20° CDB; vnější teplota 7° CDB, 6° CWB ekvivalentní délka potrubí chladiva: 7,5 m; rozdíl úrovně: 0m"]
["","","","","","","(3) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","","","","","(3) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU"]
["Venkovní jednotka","","","","","","","RZQG100L8Y1","RZQG100L8Y1","RZQG125L8Y1","RZQG125L8Y1"]
["Prostorové chlazení","Třída energetické úspornosti","","","","","","A","A++","A","A++"]
["","Kapacita","Pnávrh","kW","","","","9.50","9.50","12.0","12.0"]
["","SEER","","","","","","5.10","7.00","5.10","6.61"]
["","Roční spotřeba energie","","kWh/a","","","","652","475","824","636"]
["Prostorové vytápění (průměrné klima)","Třída energetické účinnosti","","","","","","A","A++","A","A++"]
["","Výkon","Pnávrh","kW","","","","11.30","11.30","12.71","12.66"]
["","SCOP/A","","","","","","3.80","4.80","3.80","4.63"]
["","Topný výkon Pdh při -10°","","kW","","","","9.66","9.69","11.4","11.5"]
["","Roční spotřeba energie","","kWh/a","","","","4164","3296","4683","3829"]
["Prostorové chlazení","ηs, c","","%","","","","","","","","266.9"]
["Prostorové vytápění (průměrné klima)","ηs, h","","%","","","","","","","","172.1"]