{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":7,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / AZQS-BY1 UK"]
[]
[]
[]
[]
["","","","","FCQG100FVEB / AZQS100B7Y1B UK","FCQG125FVEB / AZQS125B7Y1B UK","FCQG140FVEB / AZQS140B7Y1B UK"]
["Chladicí výkon","Jm.","","kW","9.5","12.1","13.0"]
["Prostorové chlazení","SEER","","","5.50"]
["","Roční spotřeba energie","","kWh/r","605"]
["","Kapacita","Pnávrh","kW","9.50"]
["","Třída energetické úspornosti","","","A"]
["Prostorové vytápění (průměrné klima)","Výkon","Pnávrh","kW","7.60"]
["","SCOP/A","","","3.85"]
["","Třída energetické účinnosti","","","A"]
["","Roční spotřeba energie","","kWh/r","2,764"]
["Jmenovitá účinnost","Roční spotřeba energie","","kWh","1,480","1,952","2,313"]
["","EER","","","3.21","3.10","2.81"]
["","COP","","","3.50","3.41","3.30"]
["","Směrnice o energetických štítcích","Chlazení","","A","B"]
["","","Vytápění","","B","B"]
["Topný výkon","Jm.","","kW","10.8","13.5","15.5"]
["Poznámky","","","","(1) - Roční spotřeba energie odpovídá Směrnici 2002/31/ES o uvádění spotřeby energie na energetických štítcích klimatizátorů vzduchu pro domácnost","(1) - Roční spotřeba energie odpovídá Směrnici 2002/31/ES o uvádění spotřeby energie na energetických štítcích klimatizátorů vzduchu pro domácnost","(1) - Roční spotřeba energie odpovídá Směrnici 2002/31/ES o uvádění spotřeby energie na energetických štítcích klimatizátorů vzduchu pro domácnost"]
["","","","","(2) - SEER a SCOP odpovídají EN 14825","(2) - SEER a SCOP odpovídají EN 14825","(2) - SEER a SCOP odpovídají EN 14825"]
["","","","","(3) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení","(3) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení","(3) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení"]