{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":6,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RXS-F"]
[]
[]
[]
[]
["","","","","FCQG60FVEB / RXS60F3V1B","FCQG60FVEB / RXS60F4V1B"]
["Chladicí výkon","Jm.","","kW","5.70 (3)","5.70"]
["Připojovací rozměry","Kapalina","Vnější průměr","mm","","6.35"]
["","Plyn","Vnější průměr","mm","","12.7"]
["","Odvod kondenzátu","OD","mm","","VP20 (Vnější průměr 26, Vnitřní průměr 20)"]
["Jmenovitá účinnost","Roční spotřeba energie","","kWh","820","820"]
["","EER","","","3.48","3.48"]
["","COP","","","3.52","3.52"]
["","Směrnice o energetických štítcích","Chlazení","","A","A"]
["","","Vytápění","","B","B"]
["Topný výkon","Jm.","","kW","7.00 (4)","7.00"]
["Poznámky","","","","(1) - Štítek spotřeby: stupnice od A (nejúčinnější) do G (nejméně účinné)","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU"]
["","","","","(2) - Roční spotřeba energie: počítáno podle průměrného používání po dobu 500 provozních hodin za rok při plné zátěži (= jmenovité podmínky)","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení"]
["","","","","(3) - Køling: indendørs temp: 27 °CDB, 19,0 °CWB; udendørs temp. 35°CDB; tilsvarende rørlængde: 5m, niveauforskel: 0m"]
["","","","","(4) - Varme: indendørs temp: 20 °CDB; udendørs temp. 7 °CDB, 6 °CWB; tilsvarende kølemiddelrørlængde: 5m, niveauforskel: 0m"]
["","","","","(5) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení"]