{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":13,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FCQG71FVEB / RZQSG71L3V1B","FCQG100FVEB / RZQSG100L9V1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQSG100L9V1B","FCQG50FVEB / FCQG50FVEB / RZQSG100L9V1B","FCQG125FVEB / RZQSG125L9V1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQSG125L9V1B","FCQG50FVEB / FCQG50FVEB / FCQG50FVEB / RZQSG125L9V1B","FCQG60FVEB / FCQG60FVEB / RZQSG125L9V1B","FCQG140FVEB / RZQSG140L9V1B"]
["Chladicí výkon","Jm.","","kW","6.8","9.5","","","12.0","","","","13.4"]
["Prostorové chlazení","SEER","","","6.10","6.50","5.10","5.10","5.30","4.80","4.80","4.80"]
["","Roční spotřeba energie","","kWh/rok","390","512","652","652","793","875","875","875"]
["","Kapacita","Pnávrh","kW","6.80","9.50","9.50","9.50","12.00","12.00","12.00","12.00"]
["","Třída energetické úspornosti","","","A++","A","B","B","A","B","B","B"]
["Prostorové vytápění (průměrné klima)","Výkon","Pnávrh","kW","6.33","7.60","7.60","7.60","8.03","7.60","7.60","7.60"]
["","SCOP/A","","","4.10","4.10","3.80","3.80","4.01","3.80","3.80","3.80"]
["","Třída energetické účinnosti","","","A+","B","A","A","B","A","A","A"]
["","Roční spotřeba energie","","kWh/rok","2,162","2,596","2,800","2,800","2,804","2,800","2,800","2,800"]
["Jmenovitá účinnost","Roční spotřeba energie","","kWh","1,060","1,440","","","1,870"]
["","EER","","","3.21","3.30","","","3.21","","","","3.01"]
["","COP","","","3.61","3.54","","","3.41","","","","3.41"]
["","Směrnice oenergetických štítcích","Chlazení","","A","A","","","A"]
["","","Vytápění","","A","B","","","B"]
["Topný výkon","Jm.","","kW","7.5","10.8","","","13.5","","","","15.5"]
["Poznámky","","","","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","","","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","","","","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU"]
["","","","","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení","","","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení","","","","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení"]
["","","","","","(3) - Roční spotřeba energie odpovídá Směrnici 2002/31/ES o uvádění spotřeby energie na energetických štítcích klimatizátorů vzduchu pro domácnost","","","(3) - Roční spotřeba energie odpovídá Směrnici 2002/31/ES o uvádění spotřeby energie na energetických štítcích klimatizátorů vzduchu pro domácnost"]
["","","","","","(4) - SEER a SCOP odpovídají EN 14825","","","(4) - SEER a SCOP odpovídají EN 14825"]
["","","","","","","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU"]