{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":8,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQHG-F / RZQG-L8/7V1"]
[]
[]
[]
[]
["","","","","FCQHG71FVEB / RZQG71L8V1B","FCQHG100FVEB / RZQG100L8V1B","FCQHG125FVEB / RZQG125L8V1B","FCQHG140FVEB / RZQG140L7V1B"]
["Chladicí výkon","Jm.","","kW","6.8","9.5","12.0","13.4"]
["Prostorové chlazení","SEER","","","7.00","7.00","6.61"]
["","Roční spotřeba energie","","kWh/r","340","475","635.401"]
["","Kapacita","Pnávrh","kW","6.80","9.50","12.00"]
["","Třída energetické úspornosti","","","A++","A++","A++"]
["Prostorové vytápění (průměrné klima)","Výkon","Pnávrh","kW","7.60","11.30","12.66"]
["","SCOP/A","","","4.54","4.80","4.63"]
["","Třída energetické účinnosti","","","A+","A++","A++"]
["","Roční spotřeba energie","","kWh/r","2,343","3,295.833","3,829"]
["Jmenovitá účinnost","Roční spotřeba energie","","kWh","830","1,075","1,500","2,000"]
["","EER","","","4.09","4.42","4.00","3.35"]
["","COP","","","4.80","4.99","4.40","4.12"]
["","Směrnice o energetických štítcích","Chlazení","","A","A","A"]
["","","Vytápění","","A","A","A"]
["Topný výkon","Jm.","","kW","7.5","10.8","13.5","15.5"]
["Poznámky","","","","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU"]
["","","","","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení"]