{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":117,"n_cols":9,"rows_kept":117,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQHG-F"]
[]
[]
[]
[]
["","","","","","FCQHG71FVEB","FCQHG100FVEB","FCQHG125FVEB","FCQHG140FVEB"]
["Hladina akustického tlaku","Vytápění","","Vysoké","dBA","","44","45","45"]
["","","","Jm.","dBA","","39","40","41"]
["","","","Nízký","dBA","","33","35","37"]
["","Chlazení","","Nízký","dBA","","33","35","37"]
["","","","Vysoké","dBA","","44","45","45"]
["","","","Jm.","dBA","","39","40","41"]
["Standardní příslušenství","Manuální ovládání","","","","","Manuální ovládání","Manuální ovládání","Manuální ovládání"]
["","Příručka pro instalaci","","","","","Příručka pro instalaci","Příručka pro instalaci","Příručka pro instalaci"]
["","Drenážní hadice","","","","","Drenážní hadice","Drenážní hadice","Drenážní hadice"]
["","Svorka na drenážní hadici","","","","","Svorka na drenážní hadici","Svorka na drenážní hadici","Svorka na drenážní hadici"]
["","Podložka pro konzoli závěsu","","","","","Podložka pro konzoli závěsu","Podložka pro konzoli závěsu","Podložka pro konzoli závěsu"]
["","Šrouby","","","","","Šrouby","Šrouby","Šrouby"]
["","Návod k instalaci","","","","","Návod k instalaci","Návod k instalaci","Návod k instalaci"]
["","Izolace pro upevnění","","","","","2","2","2"]
["","Těsnicí podložky","","","","","4","4","4"]
["","Těsnící podložka odvodnění","","","","","Těsnící podložka odvodnění","Těsnící podložka odvodnění","Těsnící podložka odvodnění"]
["","Svorky","","","","","Svorky","Svorky","Svorky"]
["Řídicí systémy","Wired remote control","","","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["","Infrared remote control","","","","","BRC7FA532F","BRC7FA532F","BRC7FA532F"]
["Připojovací rozměry","Kapalina","","Vnější průměr","mm","","9.52","9.52","9.52"]
["","Plyn","","Vnější průměr","mm","","15.9","15.9","15.9"]
["","Vypouštění","","","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)"]
["Dekorační panel 4","Rozměry","","Hloubka","mm","","50","50","50"]
["","","","Šířka","mm","","950","950","950"]
["","","","Výška","mm","","950","950","950"]
["","Model","","","","","BYCQ140D7W1 – Bílá s šedivými klapkami","BYCQ140D7W1 – Bílá s šedivými klapkami","BYCQ140D7W1 – Bílá s šedivými klapkami"]
["","Barva","","","","","Čistě bílá (RAL 9010)","Čistě bílá (RAL 9010)","Čistě bílá (RAL 9010)"]
["","Hmotnost","","","kg","","5.4","5.4","5.4"]
["Hladina akustického výkonu","Chlazení","","","dBA","","61","61","61"]
["","Vytápění","","","dBA","","61","61","61"]
["Rozměry","Jednotka","","Šířka","mm","","840","840","840"]
["","","","Hloubka","mm","","840","840","840"]
["","","","Výška","mm","","288","288","288"]
["Opláštění","Materiál","","","","","Pozinkovaný ocelový plech","Pozinkovaný ocelový plech","Pozinkovaný ocelový plech"]
["Hmotnost","Jednotka","","","kg","","26","26","26"]
["Dekorační panel","Hmotnost","","","kg","","10.3","10.3","10.3"]
["","Model","","","","","BYCQ140D7GFW1 – panel s automatickým čištěním s jemnou mřížkou filtru","BYCQ140D7GFW1 – panel s automatickým čištěním s jemnou mřížkou filtru","BYCQ140D7GFW1 – panel s automatickým čištěním s jemnou mřížkou filtru"]
["","Rozměry","","Výška","mm","","130","130","130"]
["","","","Hloubka","mm","","950","950","950"]
["","","","Šířka","mm","","950","950","950"]
["","Barva","","","","","Čistě bílá (RAL 9010)","Čistě bílá (RAL 9010)","Čistě bílá (RAL 9010)"]
["Power supply","Phase","","","","","1~","1~","1~"]
["","Frekvence","","","Hz","","50","50","50"]
["","Označení","","","","","VE","VE","VE"]
["","Napětí","","","V","","220-240","220-240","220-240"]
["Poznámky","","","","","","(1) - Lydeffektniveauet er en absolut værdi, som viser den styrke, som en lydkilde frembringer.","(1) - Lydeffektniveauet er en absolut værdi, som viser den styrke, som en lydkilde frembringer.","(1) - Lydeffektniveauet er en absolut værdi, som viser den styrke, som en lydkilde frembringer."]
["","","","","","","(2) - BYCQ140D7W1W má bílé izolace. Uvědomte si, že usazování nečistot na bílé izolaci je více viditelné a proto není doporučeno instalovat dekorační panel BYCQ140D7W1W v místech vystavených koncentraci nečistot.","(2) - BYCQ140D7W1W má bílé izolace. Uvědomte si, že usazování nečistot na bílé izolaci je více viditelné a proto není doporučeno instalovat dekorační panel BYCQ140D7W1W v místech vystavených koncentraci nečistot.","(2) - BYCQ140D7W1W má bílé izolace. Uvědomte si, že usazování nečistot na bílé izolaci je více viditelné a proto není doporučeno instalovat dekorační panel BYCQ140D7W1W v místech vystavených koncentraci nečistot."]
["","","","","","","(3) - BYCQ140D7W1: čistě bílý standardní panel se šedými žaluziemi; BYCQ140D7W1W: čistě bílý standardní panel s bílými žaluziemi; BYCQ140D7GW1: čistě bílý panel s automatickým čištěním.","(3) - BYCQ140D7W1: čistě bílý standardní panel se šedými žaluziemi; BYCQ140D7W1W: čistě bílý standardní panel s bílými žaluziemi; BYCQ140D7GW1: čistě bílý panel s automatickým čištěním.","(3) - BYCQ140D7W1: čistě bílý standardní panel se šedými žaluziemi; BYCQ140D7W1W: čistě bílý standardní panel s bílými žaluziemi; BYCQ140D7GW1: čistě bílý panel s automatickým čištěním."]
["Opláštění","Materiál","","","","Pozinkovaný ocelový plech"]
["Rozměry","Jednotka","","Výška","mm","288"]
["","","","Šířka","mm","840"]
["","","","Hloubka","mm","840"]
["Hmotnost","Jednotka","","","kg","25"]
["Ventilátor","Průtok vzduchu","Chlazení","Vysoké","m³/min","21.2"]
["","","","Jm.","m³/min","16.7"]
["","","","Nízký","m³/min","12.2"]
["","","Vytápění","Vysoké","m³/min","21.2"]
["","","","Jm.","m³/min","16.7"]
["","","","Nízký","m³/min","12.2"]
["Hladina akustického výkonu","Chlazení","","","dBA","53"]
["","Vytápění","","","dBA","53"]
["Hladina akustického tlaku","Chlazení","","Vysoké","dBA","36"]
["","","","Jm.","dBA","33"]
["","","","Nízký","dBA","29"]
["","Vytápění","","Vysoké","dBA","36"]
["","","","Jm.","dBA","33"]
["","","","Nízký","dBA","29"]
["Připojovací rozměry","Kapalina","","Vnější průměr","mm","9.52"]
["","Plyn","","Vnější průměr","mm","15.9"]
["","Odvod kondenzátu","","","","VP25 (I.D. 25/O.D. 32)"]
["Dekorační panel","Model","","","","BYCQ140D7GFW1 – panel s automatickým čištěním s jemnou mřížkou filtru"]
["","Barva","","","","Čistě bílá (RAL 9010)"]
["","Rozměry","","Výška","mm","130"]
["","","","Šířka","mm","950"]
["","","","Hloubka","mm","950"]
["","Hmotnost","","","kg","10.3"]
["Dekorační panel 2","Model","","","","BYCQ140D7GW1 – Panel s automatickým čištěním"]
["","Barva","","","","Čistě bílá (RAL 9010)"]
["","Rozměry","","Výška","mm","130"]
["","","","Šířka","mm","950"]
["","","","Hloubka","mm","950"]
["","Hmotnost","","","kg","10.3"]
["Dekorační panel 3","Model","","","","BYCQ140D7W1W –  Pouze bílá"]
["","Barva","","","","Čistě bílá (RAL 9010)"]
["","Rozměry","","Výška","mm","50"]
["","","","Šířka","mm","950"]
["","","","Hloubka","mm","950"]
["","Hmotnost","","","kg","5.4"]
["Dekorační panel 4","Model","","","","BYCQ140D7W1 – Bílá s šedivými klapkami"]
["","Barva","","","","Čistě bílá (RAL 9010)"]
["","Rozměry","","Výška","mm","950"]
["","","","Šířka","mm","950"]
["","","","Hloubka","mm","50"]
["","Hmotnost","","","kg","5.4"]
["Řídicí systémy","Infrared remote control","","","","BRC7FA532F"]
["Řídicí systémy","Kabelové dálkové ovládání","","","","BRC1D52, BRC1E52A/B"]
["Standardní příslušenství","Installation manual","","","","Installation manual"]
["","Washer for hanger bracket","","","","Washer for hanger bracket"]
["","Operation manual","","","","Operation manual"]
["","Clamp for drain hose","","","","Clamp for drain hose"]
["","Clamps","","","","Clamps"]
["","Drain hose","","","","Drain hose"]
["","Drain sealing pad","","","","Drain sealing pad"]
["","Installation guide","","","","Installation guide"]
["","Insulation for fitting","","","","2"]
["","Screws","","","","Screws"]
["","Sealing pads","","","","4"]
["Napájení","Označení","","","","VE"]
["","Fáze","","","","1~"]
["","Napájení-=-Frekvence","","Frekvence","","50"]
["","Napájení-=-Napětí","","Napětí","","220-240"]