{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":5,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A / RQ-BW1"]
[]
[]
[]
[]
["","","","","FDA125A5VEB / RQ125B8W1B"]
["Chladicí výkon","Jm.","","kW","12.2 (3)"]
["Jmenovitá účinnost","EER","","","2.70"]
["","Roční spotřeba energie","","kWh","2,260"]
["","COP","","","3.30"]
["","Směrnice oenergetických štítcích","Chlazení","","D"]
["","","Vytápění","","C"]
["Topný výkon","Jm.","","kW","14.5 (5)"]
["Poznámky","","","","(1) - Chlazení: vnitřní teplota 27° CDB, 19° CWB; vnější teplota 35 °CST; ekvivalentní délka potrubí: 5m; rozdíl úrovně: 0m"]
["","","","","(2) - Chlazení: vnitřní teplota 27° CDB, 19° CWB; vnější teplota 35 °CST; ekvivalentní délka potrubí: 7,5 m; rozdíl úrovně: 0m"]
["","","","","(3) - Chlazení: vnitřní teplota 27° CDB, 19° CWB; vnější teplota 35 °CST; ekvivalentní délka potrubí: 7,5 m, (vodorovné); rozdíl úrovně: 0m"]
["","","","","(4) - Varme: indendørs temp: 20 °CDB; udendørs temp. 7 °CDB, 6 °CWB; tilsvarende kølemiddelrørlængde: 5m, niveauforskel: 0m"]
["","","","","(5) - Vytápění: vnitřní teplota 20° CDB; vnější teplota 7° CDB, 6° CWB ekvivalentní délka potrubí chladiva: 7,5 m; rozdíl úrovně: 0m"]