{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":67,"n_cols":8,"rows_kept":67,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A"]
[]
[]
[]
[]
["","","","","","FDA125A5VEB","FDA200AXVEB","FDA250AXVEB"]
["Chladicí výkon","Celkový výkon","","Jm.","kW","12.10","19.00","22.00"]
["Topný výkon","Celkový výkon","","Jmen.","kW","13.50","22.4","24.0"]
["Opláštění","Barva","","","","Nelakovaný","Nelakovaný","Nelakovaný"]
["","Materiál","","","","Pozinkovaná ocel","Pozinkovaný ocelový plech","Pozinkovaný ocelový plech"]
["Rozměry","Jednotka","","Výška","mm","300","470","470"]
["","","","Šířka","mm","1,400","1,490","1,490"]
["","","","Hloubka","mm","700","1,100","1,100"]
["Hmotnost","Jednotka","","","kg","45","104","115"]
["Požadovaná výška podstropení >","mm","","","","350"]
["Ventilátor","Průtok vzduchu","Chlazení","Vysoké","m³/min","39.0","64.0","69.0"]
["","","","Střední","m³/min","","50","56"]
["","","","Nízký","m³/min","28.0","36.0","43.0"]
["","","Vytápění","Vysoké","m³/min","39.0","64.0","69.0"]
["","","","Střední","m³/min","","50.0","56.0"]
["","","","Nízký","m³/min","28.0","36.0","43.0"]
["","Vnější statický tlak","","Vysoký","Pa","200","250","250"]
["","","","Jmen.","Pa","50","62","62"]
["Hladina akustického výkonu","Chlazení","","","dBA","66","69.0","71.0"]
["Hladina akustického tlaku","Chlazení","","Vysoké","dBA","40","43.0","44.0"]
["","","","Střední","dBA","","39.0","40.0"]
["","","","Nízký","dBA","33","36.0","37.0"]
["","Vytápění","","Vysoké","dBA","40","43.0","44.0"]
["","","","Střední","dBA","","39.0","40.0"]
["","","","Nízký","dBA","33","36.0","37.0"]
["Připojovací rozměry","Kapalina","","Vnější průměr","mm","9.52","9.52","9.52"]
["","Plyn","","Vnější průměr","mm","15.90","19.1","22.2"]
["","Vypouštění","","","","VP25 (I.D. 25/O.D. 32)","BSP1","BSP1"]
["Hladina vypouštění","mm","","","","625"]
["Dekorační panel","Model","","","","BYBS125DJW1"]
["","Barva","","","","Bílá (10Y9/0,5)"]
["","Rozměry","","Výška","mm","55"]
["","","","Šířka","mm","1,500"]
["","","","Hloubka","mm","500"]
["","Hmotnost","","","kg","6.5"]
["Control systems","Infrared remote control","","","","BRC4C65, BRC4C66"]
["","Wired remote control","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Standardní příslušenství","Šrouby","","","","16","2","2"]
["","Podložka","","","","8","12","12"]
["","Hadicová páska","","","","1"]
["","Drenážní hadice","","","","1"]
["","Obecná bezpečnostní opatření","","","","1","1","1"]
["","Příručka pro montáž a provoz","","","","1","1","1"]
["","Kabel pro běžný napájecí zdroj","","","","2"]
["","Těsnicí materiál (odtoková hadice)","","","","1"]
["","Těsnící materiál","","","","2"]
["","Tepelná izolační trubka (kapalina)","","","","1"]
["","Tepelná izolační trubka (plyn)","","","","1"]
["Power supply","Označení","","","","","VE","VE"]
["","Fáze","","","","1~","1~","1~"]
["","Frekvence","","","Hz","50/60","50/60","50/60"]
["","Napětí","","","V","220-240/220","220-240/220","220-240/220"]
["Poznámky","","","","","(1) - Údaje o elektrickém systému najdete v samostatném výkresu"]
["Standardní příslušenství","Manuální ovládání","","","","","1","1"]
["","Příručka pro instalaci","","","","","1","1"]
["","Připojovací trubka plynu","","","","","1","1"]
["","Materiál svorky vodiče","","","","","1","1"]
["","Pružná podložka","","","","","2","2"]
["","Šroub + podložka","","","","","45","45"]
["","Šroub s šestihrannou hlavou s podložkou","","","","","49","49"]
["","Šroub s šestihrannou hlavou","","","","","2","2"]
["","Plochá podložka","","","","","8","8"]