{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDBQ-B"]
[]
[]
[]
[]
["","","","","","FDBQ25B5V1","FDBQ25B8V1"]
["Hladina akustického tlaku","Vytápění","","Vysoké","dBA","35.0","35.0"]
["","","","Nízký","dBA","29.0","29.0"]
["","Chlazení","","Nízký","dBA","28.0","28.0"]
["","","","Vysoké","dBA","35.0","35.0"]
["Standardní příslušenství","Příručka pro montáž a provoz","","","","1","1"]
["","Filtr sání vzduchu","","","","1","1"]
["Řídicí systémy","Wired remote control","","","","BRC1D52, BRC1E52A/B"]
["Spoje potrubí","Liquid","","OD","mm","6.35"]
["","Plyn","","OD","mm","9.52"]
["","Vypouštění","","","","27.2"]
["Hladina akustického výkonu","Chlazení","","","dBA","55","55"]
["","Vytápění","","","dBA","55","55"]
["Rozměry","Jednotka","","Šířka","mm","652","652"]
["","","","Hloubka","mm","502","502"]
["","","","Výška","mm","230","230"]
["Casing","Material","","","","Pozinkovaná nízkouhlíková ocel","Pozinkovaná nízkouhlíková ocel"]
["Hmotnost","Jednotka","","","kg","17.0","17.0"]
["Fan","Průtok vzduchu","Vytápění","Vysoké","m³/min","","6.95"]
["","","","Nízký","m³/min","","5.20"]
["","","Chlazení","Nízký","m³/min","","5.20"]
["","","","Vysoké","m³/min","","6.50"]
["Power supply","Fáze","","","","1~","1~"]
["","Frekvence","","","Hz","50","50"]
["","Name","","","","V1","V1"]
["","Napětí","","","V","230","230 +/-10%"]
["Poznámky","","","","","(1) - Hodnoty zvuku jsou měřeny v akusticky polomrtvé komoře.","(1) - Hodnoty zvuku jsou měřeny v akusticky polomrtvé komoře."]
["","","","","","(2) - Hladina akustického tlaku je relativní hodnota závislá na vzdálenosti a akustickém prostředí. Další podrobnosti naleznete na výkresech s hlukovými údaji.","(2) - Hladina akustického tlaku je relativní hodnota závislá na vzdálenosti a akustickém prostředí. Další podrobnosti naleznete na výkresech s hlukovými údaji."]
["","","","","","(3) - Lydeffektniveauet er en absolut værdi, som viser den styrke, som en lydkilde frembringer.","(3) - Lydeffektniveauet er en absolut værdi, som viser den styrke, som en lydkilde frembringer."]
["Spoje potrubí","Liquid","","OD","mm","","6.35"]
["","Plyn","","OD","mm","","9.52"]
["","Vypouštění","","","","","27.2"]