{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-B / RZQ-D3/D9V1"]
[]
[]
[]
[]
["","","","","FDQ125B8V3B9 / RZQ125D9V1B"]
["Chladicí výkon","Jm.","","kW","12.5 (3)"]
["Piping connections","Kapalina","Vnější průměr","mm","9.52"]
["","Plyn","Vnější průměr","mm","15.9"]
["","Vypouštění","OD","mm","26"]
["Prostorové chlazení","SEER","","","3.50"]
["Jmenovitá účinnost","Roční spotřeba energie","","kWh","1,978"]
["","EER","","","3.16"]
["","COP","","","3.88"]
["","Směrnice oenergetických štítcích","Chlazení","","B"]
["","","Vytápění","","A"]
["Topný výkon","Jm.","","kW","14.0 (4)"]
["Poznámky","","","","(1) - Štítek spotřeby: stupnice od A (nejúčinnější) do G (nejméně účinné)"]
["","","","","(2) - Roční spotřeba energie: počítáno podle průměrného používání po dobu 500 provozních hodin za rok při plné zátěži (= jmenovité podmínky)"]
["","","","","(3) - Chlazení: vnitřní teplota 27° CDB, 19° CWB; vnější teplota 35 °CST; ekvivalentní délka potrubí: 5m; rozdíl úrovně: 0m"]
["","","","","(4) - Varme: indendørs temp: 20 °CDB; udendørs temp. 7 °CDB, 6 °CWB; tilsvarende kølemiddelrørlængde: 5m, niveauforskel: 0m"]
["","","","","(5) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení"]