{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":6,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-C / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FDQ125C5VEB / RZQG125L8Y1B","FDQ125C7VEB / RZQG125L8Y1B"]
["Chladicí výkon","Jm.","","kW","12.0","12.0"]
["Prostorové chlazení","SEER","","","5.81","5.81"]
["","Roční spotřeba energie","","kWh/r","723","723"]
["","Kapacita","Pnávrh","kW","12","12"]
["","Třída energetické úspornosti","","","A+","A+"]
["Prostorové vytápění (průměrné klima)","Výkon","Pnávrh","kW","12.71","12.71"]
["","SCOP/A","","","4.21","4.21"]
["","Třída energetické účinnosti","","","A+","A+"]
["","Roční spotřeba energie","","kWh/r","4,227","4,227"]
["Jmenovitá účinnost","Roční spotřeba energie","","kWh","1,600","1,600"]
["","EER","","","3.75","3.75"]
["","COP","","","3.83","3.83"]
["","Směrnice o energetických štítcích","Chlazení","","A","A"]
["","","Vytápění","","A","A"]
["Topný výkon","Jm.","","kW","13.5","13.5"]
["Poznámky","","","","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU"]
["","","","","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení"]