{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":6,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-C / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FDQ125C5VEB / RZQSG125L9V1B (Archived)","FDQ125C7VEB / RZQSG125L9V1B (Archived)"]
["Chladicí výkon","Jm.","","kW","12.0","12.0"]
["Topný výkon","Jm.","","kW","13.5","13.5"]
["Jmenovitá účinnost","EER","","","3.21","3.21"]
["","COP","","","3.51","3.51"]
["","Annual energy consumption","","kWh","1,870","1,870"]
["","Směrnice o energetických štítcích","Chlazení","","A","A"]
["","","Vytápění","","B","B"]
["Prostorové chlazení","Třída energetické úspornosti","","","A","A"]
["","Kapacita","Pnávrh","kW","12.00","12.00"]
["","SEER","","","5.20","5.20"]
["","Roční spotřeba energie","","kWh/r","808","808"]
["Prostorové vytápění (průměrné klima)","Třída energetické účinnosti","","","A","A"]
["","Výkon","Pnávrh","kW","7.60","7.60"]
["","SCOP/A","","","3.90","3.90"]
["","Roční spotřeba energie","","kWh/r","2,729","2,729"]
["Poznámky","","","","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU"]
["","","","","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení"]