{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":6,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-C"]
[]
[]
[]
[]
["","","","","FDQ125C5VEB","FDQ125C7VEB"]
["Hladina akustického tlaku","Vytápění","Vysoké","dBA","40","40"]
["","","Nízký","dBA","33","33"]
["","Chlazení","Nízký","dBA","33","33"]
["","","Vysoké","dBA","40","40"]
["Control systems","Wired remote control","","","BRC1D52, BRC1E53A, BRC1E53B, BRC1E53C","BRC1D52, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D528"]
["","Infračervené dálkové ovládání","","","BRC4C65","BRC4C65"]
["Chladicí výkon","Celkový výkon","Jm.","kW","12.5 (1)","12.5"]
["Spoje potrubí","Kapalný","OD","mm","9.52","9.52"]
["","Plyn","OD","mm","15.9","15.9"]
["","Drain","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)"]
["Vstup napájení","Chlazení","Jm.","kW","0.35"]
["","Vytápění","Jm.","kW","0.35"]
["Požadovaná výška podstropení >","mm","","","350","350"]
["Hladina akustického výkonu","Chlazení","","dBA","66","66"]
["Rozměry","Unit","Width","mm","1,400","1,400"]
["","","Depth","mm","700","700"]
["","","Height","mm","300","300"]
["Opláštění","Materiál","","","","Pozinkovaná ocel"]
["","Barva","","","Nenatřeno (pozinkováno)","Not painted"]
["Hmotnost","Unit","","kg","45","45"]
["Ventilátor","Vnější statický tlak","Vysoký","Pa","200","200"]
["","","Jmen.","Pa","50","50"]
["Hladina vypouštění","mm","","","625","625"]
["Dekorační panel","Hmotnost","","kg","6.5","6.5"]
["","Model","","","BYBS125DJW1","BYBS125DJW1"]
["","Rozměry","Výška","mm","55","55"]
["","","Hloubka","mm","500","500"]
["","","Šířka","mm","1,500","1,500"]
["","Barva","","","Bílá (10Y9/0,5)","Bílá (10Y9/0,5)"]
["Topný výkon","Celkový výkon","Jmen.","kW","14.0 (2)","14.0"]
["Power supply","Fáze","","","1~","1~"]
["","Frekvence","","Hz","50/60","50/60"]
["","Označení","","","VE","VE"]
["","Napětí","","V","220-240/220","220-240/220"]
["Poznámky","","","","(1) - Chlazení pokojová teplota 27°CDB, 19,0°CWB; venkovní teplota 35°CDB; ekvivalentní délka potrubí: 7,5m; rozdíl hladin: 0m","(1) - Vytápění: vnitřní teplota 20° CDB; vnější teplota 7° CDB, 6° CWB ekvivalentní délka potrubí chladiva: 7,5 m; rozdíl úrovně: 0m"]
["","","","","(2) - Vytápění: vnitřní teplota 20° CDB; vnější teplota 7° CDB, 6° CWB ekvivalentní délka potrubí chladiva: 7,5 m; rozdíl úrovně: 0m","(2) - Kapaciteterne er nettoværdier inklusive fradrag for afkøling (og tillæg for opvarmning) for den indendørs ventilators motorvarme."]
["","","","","(3) - Kapaciteterne er nettoværdier inklusive fradrag for afkøling (og tillæg for opvarmning) for den indendørs ventilators motorvarme.","(3) - Lydtryksværdierne nævnes for en enhed, der er monteret med udsugning bagpå."]
["","","","","(4) - Lydtryksværdierne nævnes for en enhed, der er monteret med udsugning bagpå.","(4) - Kategorie PED jednotky: vyjmuto z rozsahu PED kvůli čl. 1, pol. 3.6 z 97/23/ES"]
["","","","","(5) - Kategorie PED jednotky: vyjmuto z rozsahu PED kvůli čl. 1, pol. 3.6 z 97/23/ES","(5) - Chlazení: vnitřní teplota 27° CDB, 19° CWB; vnější teplota 35 °CST; ekvivalentní délka potrubí: 7,5 m, (vodorovné); rozdíl úrovně: 0m"]