{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":6,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3 / 2MXM-M"]
[]
[]
[]
[]
["","","","","FDXM25F3V1B / FDXM25F3V1B / 2MXM40M3V1B","FDXM25F3V1B / FDXM35F3V1B / 2MXM40M3V1B"]
["Chladicí výkon","Jm.","","kW","4.0","4.0"]
["Jmenovitá účinnost","Annual energy consumption","","kWh","563","555"]
["","EER","","","3.55","3.60"]
["","COP","","","4.13","4.17"]
["","Směrnice o energetických štítcích","Chlazení","","A","A"]
["","","Vytápění","","A","A"]
["Topný výkon","Jm.","","kW","4.20","4.20"]
["Poznámky","","","","(1) - Jmenovité chladící výkony jsou založeny na: vnitřní teplota: 27 °CST, 19 °CMT, venkovní teplota: 35 °CST, ekvivalentní délka potrubí chladiva: 5 m, rozdíl úrovní: 0 m. Data pro řadu se standardní účinností","(1) - Jmenovité chladící výkony jsou založeny na: vnitřní teplota: 27 °CST, 19 °CMT, venkovní teplota: 35 °CST, ekvivalentní délka potrubí chladiva: 5 m, rozdíl úrovní: 0 m. Data pro řadu se standardní účinností"]
["","","","","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m.","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m."]