{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":9,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9"]
[]
[]
[]
[]
["","","","","","FDXM25F3V1B9","FDXM35F3V1B9","FDXM50F3V1B9","FDXM60F3V1B9"]
["Hladina akustického tlaku","Vytápění","","Vysoké","dBA","35.0","35.0","","38.0"]
["","","","Střední","dBA","33.0","33.0","","35.0"]
["","","","Nízký","dBA","27.0","27.0","","30.0"]
["","Chlazení","","Střední","dBA","33.0","33.0","","35.0"]
["","","","Nízký","dBA","27.0","27.0","","30.0"]
["","","","Vysoké","dBA","35.0","35.0","","38.0"]
["Standardní příslušenství","Příručka pro instalaci","","","","1","1","","1"]
["","Manuální ovládání","","","","1","1","","1"]
["","Izolace pro upevnění","","","","1","1","","1"]
["","Těsnicí podložky","","","","1","1","","1"]
["","Kovová svorka","","","","1","1","","1"]
["","Drenážní hadice","","","","1","1","","1"]
["","Podložka pro konzoli závěsu","","","","8","8","","8"]
["","Těsnící materiál","","","","2","2","","2"]
["","Svorky","","","","6","6","","6"]
["","Upínací deska podložky","","","","4","4","","4"]
["","Šrouby pro příruby kanálu","","","","1","1","","1"]
["","Vzduchový filtr","","","","1","1","","1"]
["Připojovací rozměry","Kapalina","","Vnější průměr","mm","6.35","6.35","","6.35"]
["","Plyn","","Vnější průměr","mm","9.50","9.50","","12.70"]
["","Vypouštění","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","","VP20 (I.D. 20/O.D. 26)"]
["Vstup napájení","Chlazení","","Jm.","kW","0.036","0.036","","0.060"]
["","Vytápění","","Jm.","kW","0.036","0.036","","0.060"]
["Hladina akustického výkonu","Chlazení","","","dBA","53.0","53.0","","56.0"]
["","Vytápění","","","dBA","53.0","53.0","","56.0"]
["Rozměry","Jednotka","","Šířka","mm","750","750","","1,150"]
["","","","Hloubka","mm","620","620","","620"]
["","","","Výška","mm","200","200","","200"]
["Hmotnost","Jednotka","","","kg","21","21","","28"]
["Ventilátor","Vnější statický tlak","","Jmen.","Pa","30","30","","40"]
["","Průtok vzduchu","Vytápění","Vysoké","m³/min","8.7","8.7","","16.0"]
["","","","Střední","m³/min","8.0","8.0","","14.8"]
["","","","Nízký","m³/min","7.3","7.3","","13.5"]
["","","Chlazení","Nízký","m³/min","7.3","7.3","","13.5"]
["","","","Střední","m³/min","8.0","8.0","","14.8"]
["","","","Vysoké","m³/min","8.7","8.7","","16.0"]
["Power supply","Phase","","","","1~","1~","","1~"]
["","Frekvence","","","Hz","50","50","","50"]
["","Napětí","","","V","220-240","220-240","","220-240"]
["Poznámky","","","","","(1) - Údaje o elektrickém systému najdete v samostatném výkresu","(1) - Údaje o elektrickém systému najdete v samostatném výkresu","","(1) - Údaje o elektrickém systému najdete v samostatném výkresu"]
["Vstup napájení","Chlazení","","Jm.","kW","","","0.060"]
["","Vytápění","","Jm.","kW","","","0.060"]
["Rozměry","Jednotka","","Výška","mm","","","200"]
["","","","Šířka","mm","","","1150"]
["","","","Hloubka","mm","","","620"]
["Hmotnost","Jednotka","","","kg","","","28"]
["Ventilátor","Průtok vzduchu","Chlazení","Vysoké","m³/min","","","15.8"]
["","","","Střední","m³/min","","","14.6"]
["","","","Nízký","m³/min","","","13.3"]
["","","Vytápění","Vysoké","m³/min","","","15.8"]
["","","","Střední","m³/min","","","14.6"]
["","","","Nízký","m³/min","","","13.3"]
["","Vnější statický tlak","","Jmen.","Pa","","","40"]
["Hladina akustického výkonu","Chlazení","","","dBA","","","55.0"]
["","Vytápění","","","dBA","","","55.0"]
["Hladina akustického tlaku","Chlazení","","Vysoké","dBA","","","38.0"]
["","","","Střední","dBA","","","35.0"]
["","","","Nízký","dBA","","","30.0"]
["","Vytápění","","Vysoké","dBA","","","38.0"]
["","","","Střední","dBA","","","35.0"]
["","","","Nízký","dBA","","","30.0"]
["Připojovací rozměry","Kapalina","","Vnější průměr","mm","","","6.35"]
["","Plyn","","Vnější průměr","mm","","","12.70"]
["","Odvod kondenzátu","","","","","","VP20 (I.D. 20/O.D. 26)"]
["Standardní příslušenství","Installation manual","","","","","","1"]
["","Washer for hanger bracket","","","","","","8"]
["","Operation manual","","","","","","1"]
["","Clamp metal","","","","","","1"]
["","Clamps","","","","","","6"]
["","Drain hose","","","","","","1"]
["","Air filter","","","","","","1"]
["","Insulation for fitting","","","","","","1"]
["","Screws for duct flanges","","","","","","1"]
["","Sealing material","","","","","","2"]
["","Sealing pad","","","","","","1"]
["","Washer fixing plate","","","","","","4"]
["Napájení","Fáze","","","","","","1~"]
["","Frekvence","","","Hz","","","50"]
["","Napětí","","","V","","","220-240"]