{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-C / RXS-F"]
[]
[]
[]
[]
["","","","","FDXS60CVMB / RXS60F3V1B"]
["Chladicí výkon","Min.","","kW","1.7"]
["","Max.","","kW","6.5"]
["","Jm.","","kW","6.0 (1)"]
["Piping connections","Kapalina","Vnější průměr","mm","6.35"]
["","Plyn","Vnější průměr","mm","12.7"]
["","Vypouštění","OD","mm","26"]
["Jmenovitá účinnost","Roční spotřeba energie","","kWh","1,065"]
["","EER","","","2.82"]
["","COP","","","3.02"]
["","Směrnice oenergetických štítcích","Chlazení","","C"]
["","","Vytápění","","D"]
["Topný výkon","Jm.","","kW","7.0 (2)"]
["","Min.","","kW","1.7"]
["","Max.","","kW","8.0"]
["Poznámky","","","","(1) - Køling: indendørs temp: 27 °CDB, 19 °CWB, udendørs temp. 35°CDB, 24°CWB; tilsvarende rørlængde: 7,5m"]
["","","","","(2) - Vytápění: vnitřní teplota 20° CDB; vnější teplota 7° CDB, 6° CWB ekvivalentní délka potrubí chladiva: 7,5m"]
["","","","","(3) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení"]