{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":7,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F / RXS-L"]
[]
[]
[]
[]
["","","","","FDXS25F2VEB / RXS25L2V1B","FDXS35F2VEB / RXS35L2V1B","FDXS60F2VEB / RXS60L2V1B"]
["Chladicí výkon","Min.","","kW","1.3","1.4","1.7"]
["","Max.","","kW","3.0","3.8","6.5"]
["","Jm.","","kW","2.4","3.4","6.0"]
["Spoje potrubí","Liquid","OD","mm","6.35","6.35","6.35"]
["","Plyn","OD","mm","9.5","9.5","12.7"]
["","Drain","OD","mm","VP20 (Vnější průměr 26, Vnitřní průměr 20)","VP20 (Vnější průměr 26, Vnitřní průměr 20)","VP20 (Vnější průměr 26, Vnitřní průměr 20)"]
["Jmenovitá účinnost","Annual energy consumption","","kWh","325","530","1,030"]
["","EER","","","3.69","3.21","2.91"]
["","COP","","","4.00","3.48","3.21"]
["","Směrnice o energetických štítcích","Chlazení","","A","A","C"]
["","","Vytápění","","A","B","C"]
["Topný výkon","Jm.","","kW","3.2","4.0","7.0"]
["","Min.","","kW","1.3","1.4","1.7"]
["","Max.","","kW","4.5","5.0","8.0"]
["Poznámky","","","","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU"]
["","","","","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","(3) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení","(3) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení","(3) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení"]