{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":6,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A / RXS-L3"]
[]
[]
[]
[]
["","","","","FFA25A2VEB / RXS25L3V1B","FFA35A2VEB / RXS35L3V1B"]
["Chladicí výkon","Jm.","","kW","2.50","3.40"]
["Prostorové chlazení","SEER","","","6.11","6.32"]
["","Roční spotřeba energie","","kWh/a","143","188"]
["","Kapacita","Pnávrh","kW","2.50","3.40"]
["","Třída energetické úspornosti","","","A++","A++"]
["Prostorové vytápění (průměrné klima)","Výkon","Pnávrh","kW","2.31","3.10"]
["","SCOP/A","","","4.24","4.10"]
["","Třída energetické účinnosti","","","A+","A+"]
["","Roční spotřeba energie","","kWh/a","763","1,059"]
["Připojovací rozměry","Kapalina","Vnější průměr","mm","6.35","6.35"]
["","Plyn","Vnější průměr","mm","9.50","9.50"]
["","Vypouštění","OD","mm","VP20 (Vnější průměr 26, Vnitřní průměr 20)","VP20 (Vnější průměr 26, Vnitřní průměr 20)"]
["Jmenovitá účinnost","EER","","","4.53","3.78"]
["","Roční spotřeba energie","","kWh","276","450"]
["","COP","","","3.90","3.50"]
["","Směrnice o energetických štítcích","Chlazení","","A","A"]
["","","Vytápění","","A","A"]
["Topný výkon","Jm.","","kW","3.20","4.20"]
["Poznámky","","","","(1) - Jmenovité chladicí výkony vycházejí z těchto podmínek: vnitřní teplota: 27°CDB, 19°CWB, venkovní teplota: 35 °CDB, ekvivalentní délka potrubí s chladivem: 5 m, rozdíl úrovní: 0 m.","(1) - Jmenovité chladicí výkony vycházejí z těchto podmínek: vnitřní teplota: 27°CDB, 19°CWB, venkovní teplota: 35 °CDB, ekvivalentní délka potrubí s chladivem: 5 m, rozdíl úrovní: 0 m."]
["","","","","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m.","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m."]
["","","","","(3) - Viz samostatný výkres s provozním rozsahem","(3) - Viz samostatný výkres s provozním rozsahem"]
["","","","","(4) - Údaje o elektrickém systému najdete v samostatném výkresu","(4) - Údaje o elektrickém systému najdete v samostatném výkresu"]