{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":7,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A / RZASG-MV1"]
[]
[]
[]
[]
["","","","","FFA35A2VEB / FFA35A2VEB / RZASG71M2V1B","FFA35A2VEB / FFA35A2VEB / FFA35A2VEB / RZASG100M7V1B","FFA50A2VEB / FFA50A2VEB / RZASG100M7V1B"]
["Chladicí výkon","Jm.","","kW","6.80 (1)"]
["Prostorové chlazení","SEER","","","6.12"]
["","Roční spotřeba energie","","kWh/rok","389"]
["","Kapacita","Pnávrh","kW","6.80"]
["","Třída energetické úspornosti","","","A++"]
["Prostorové vytápění (průměrné klima)","Výkon","Pnávrh","kW","4.50"]
["","SCOP/A","","","3.84"]
["","Třída energetické účinnosti","","","A"]
["","Roční spotřeba energie","","kWh/rok","1,641"]
["Topný výkon","Jm.","","kW","7.50 (2)"]
["Poznámky","","","","(1) - Chlazení: T2: vnitřní teplota 26,6 °CST, 19,4 °CMT, venkovní teplota 48 °CST [Btu/h/W]","(1) - Jmenovité chladicí výkony vycházejí z těchto podmínek: vnitřní tep.: 27°CDB, 19°CWB, venkovní teplota: 35 °CDB, ekvivalentní délka potrubí s chladivem: 5 m, rozdíl úrovní: 0 m.","(1) - Jmenovité chladicí výkony vycházejí z těchto podmínek: vnitřní tep.: 27°CDB, 19°CWB, venkovní teplota: 35 °CDB, ekvivalentní délka potrubí s chladivem: 5 m, rozdíl úrovní: 0 m."]
["","","","","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m.","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m.","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m."]
["Venkovní jednotka","","","","","RZASG100M7V1B","RZASG100M7V1B"]
["Chladicí výkon","Jm.","","kW","","9.50","9.50"]
["Topný výkon","Jm.","","kW","","10.8","10.8"]
["Prostorové chlazení","Třída energetické úspornosti","","","","A++","A"]
["","Kapacita","Pnávrh","kW","","9.50","9.50"]
["","SEER","","","","6.24","5.49"]
["","Roční spotřeba energie","","kWh/rok","","533","606"]
["Prostorové vytápění (průměrné klima)","Třída energetické účinnosti","","","","A","A"]
["","Výkon","Pnávrh","kW","","6.00","6.00"]
["","SCOP/A","","","","3.82","3.90"]
["","Roční spotřeba energie","","kWh/rok","","2199","2154"]