{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":6,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A9 / RXM-N"]
[]
[]
[]
[]
["","","","","FFA50A2VEB9 / RXM50N2V1B","FFA60A2VEB9 / RXM60N2V1B"]
["Chladicí výkon","Jm.","","kW","5.00"]
["Jmenovitá účinnost","Roční spotřeba energie","","kWh","772"]
["","EER","","","3.24"]
["","COP","","","3.49"]
["","Směrnice oenergetických štítcích","Chlazení","","A"]
["","","Vytápění","","A"]
["Topný výkon","Jm.","","kW","5.80"]
["Poznámky","","","","(1) - Jmenovité chladicí výkony vycházejí z těchto podmínek: vnitřní teplota: 27°CDB, 19°CWB, venkovní teplota: 35 °CDB, ekvivalentní délka potrubí s chladivem: 5 m, rozdíl úrovní: 0 m.","(1) - Jmenovité chladicí výkony vycházejí ztěchto podmínek: vnitřní tep.: 27°CDB, 19°CWB, venkovní teplota: 35°CDB, ekvivalentní délka potrubí schladivem: 5m, rozdíl úrovní: 0m."]
["","","","","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m.","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m."]
["","","","","(3) - Viz samostatný výkres s provozním rozsahem","(3) - Viz samostatný výkres s provozním rozsahem"]
["","","","","(4) - Údaje o elektrickém systému najdete v samostatném výkresu","(4) - Údaje o elektrickém systému najdete v samostatném výkresu"]
["Venkovní jednotka","","","","","RXM60N2V1B"]
["Chladicí výkon","Jm.","","kW","","5.70"]
["Topný výkon","Jm.","","kW","","7.00"]
["Jmenovitá účinnost","EER","","","","3.05"]
["","COP","","","","3.41"]
["","Roční spotřeba energie","","kWh","","934"]
["","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích-=-Chlazení","","","B"]
["","","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích-=-Vytápění","","","B"]
["Prostorové chlazení","Třída energetické úspornosti","","","","A+"]
["","Kapacita","Pnávrh","kW","","5.70"]
["","SEER","","","","5.76"]
["","Roční spotřeba energie","","kWh/a","","347"]
["Prostorové vytápění (průměrné klima)","Třída energetické účinnosti","","","","A+"]
["","Výkon","Pnávrh","kW","","3.96"]
["","SCOP/A","","","","4.04"]
["","Topný výkon Pdh při -10°","","kW","","3.66"]
["","Roční spotřeba energie","","kWh/a","","1372"]
["Energetickou účinná řada","","","","","A+++ ~ D"]