{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":14,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A9 / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / RZQG100L8Y1B","FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / RZQG125L8Y1B","FFA50A2VEB9 / FFA50A2VEB9 / FFA50A2VEB9 / RZQG125L8Y1B","FFA50A2VEB9 / FFA50A2VEB9 / RZQG100L8Y1B","FFA60A2VEB9 / FFA60A2VEB9 / RZQG125L8Y1B","FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / RZQG100L8Y1B","FFA50A2VEB9 / FFA50A2VEB9 / FFA50A2VEB9 / RZQG100L8Y1B","FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / RZQG71L8Y1B","FFA35A2VEB9 / FFA35A2VEB9 / RZQG71L8Y1B","FFA50A2VEB9 / FFA50A2VEB9 / RZQG71L8Y1B"]
["Energetickou účinná řada","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Chladicí výkon","Jm.","","kW","","","","","","","","6.80","6.80","6.80"]
["Prostorové chlazení","SEER","","","","","","","","","","5.10","5.10","5.10"]
["","Roční spotřeba energie","","kWh/r","","","","","","","","467","467","467"]
["","Kapacita","Pnávrh","kW","","","","","","","","6.80","6.80","6.80"]
["","Třída energetické úspornosti","","","","","","","","","","A","A","A"]
["Prostorové vytápění (průměrné klima)","Výkon","Pnávrh","kW","","","","","","","","6.00","6.00","6.00"]
["","SCOP/A","","","","","","","","","","3.80","3.80","3.80"]
["","Třída energetické účinnosti","","","","","","","","","","A","A","A"]
["","Roční spotřeba energie","","kWh/r","","","","","","","","2,211","2,211","2,211"]
["Jmenovitá účinnost","EER","","","","","","","","","","3.38","3.38","3.38"]
["Poznámky","","","","","","","","","","","(1) - Viz samostatný výkres s provozním rozsahem","(1) - Jmenovité chladicí výkony vycházejí z těchto podmínek: vnitřní teplota: 27°CDB, 19°CWB, venkovní teplota: 35 °CDB, ekvivalentní délka potrubí s chladivem: 5 m, rozdíl úrovní: 0 m.","(1) - Viz samostatný výkres s provozním rozsahem"]
["","","","","","","","","","","","(2) - Údaje o elektrickém systému najdete v samostatném výkresu","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m.","(2) - Údaje o elektrickém systému najdete v samostatném výkresu"]
["","","","","","","","","","","","","(3) - Viz samostatný výkres s provozním rozsahem"]
["","","","","","","","","","","","","(4) - Údaje o elektrickém systému najdete v samostatném výkresu"]