{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":64,"n_cols":9,"rows_kept":64,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A9"]
[]
[]
[]
[]
["","","","","","FFA25A2VEB9","FFA35A2VEB9","FFA50A2VEB9","FFA60A2VEB9"]
["Opláštění","Materiál","","","","Pozinkovaný ocelový plech","Pozinkovaný ocelový plech","Pozinkovaný ocelový plech","Pozinkovaný ocelový plech"]
["Rozměry","Jednotka","","Výška","mm","260","260","260","260"]
["","","","Šířka","mm","575","575","575","575"]
["","","","Hloubka","mm","575","575","575","575"]
["Hmotnost","Jednotka","","","kg","16.0","16.0","17.5","17.5"]
["Ventilátor","Průtok vzduchu","Chlazení","Vysoké","m³/min","9.0","10.0","12.7","14.5"]
["","","","Střední","m³/min","8.0","8.5","10.9","12.5"]
["","","","Nízký","m³/min","6.5","6.5","8.6","9.5"]
["","","Vytápění","Vysoké","m³/min","9.0","10.0","12.7","14.5"]
["","","","Střední","m³/min","8.0","8.5","10.9","12.5"]
["","","","Nízký","m³/min","6.5","6.5","8.6","9.5"]
["Hladina akustického výkonu","Chlazení","","","dBA","48.0","51.0","56.0","60.0"]
["Hladina akustického tlaku","Chlazení","","Vysoké","dBA","31.0","34.0","39.0","43.0"]
["","","","Střední","dBA","28.5","30.5","34.0","40.0"]
["","","","Nízký","dBA","25.0","25.0","27.0","32.0"]
["","Vytápění","","Vysoké","dBA","31.0","34.0","39.0","43.0"]
["","","","Střední","dBA","28.5","30.5","34.0","40.0"]
["","","","Nízký","dBA","25.0","25.0","27.0","32.0"]
["Připojovací rozměry","Kapalina","","Vnější průměr","mm","6","6","6","6"]
["","Plyn","","Vnější průměr","mm","9.52","9.52","12.70","12.70"]
["","Odvod kondenzátu","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Dekorační panel","Model","","","","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W"]
["","Barva","","","","Bílá (N9.5)","Bílá (N9.5)","Bílá (N9.5)","Bílá (N9.5)"]
["","Rozměry","","Výška","mm","46","46","46","46"]
["","","","Šířka","mm","620","620","620","620"]
["","","","Hloubka","mm","620","620","620","620"]
["","Hmotnost","","","kg","2.8","2.8","2.8","2.8"]
["Dekorační panel 2","Model","","","","BYFQ60C2W1S","BYFQ60C2W1S","BYFQ60C2W1S","BYFQ60C2W1S"]
["","Barva","","","","Stříbrný","Stříbrný","Stříbrný","Stříbrný"]
["","Rozměry","","Výška","mm","46","46","46","46"]
["","","","Šířka","mm","620","620","620","620"]
["","","","Hloubka","mm","620","620","620","620"]
["","Hmotnost","","","kg","2.8","2.8","2.8","2.8"]
["Dekorační panel 3","Model","","","","BYFQ60B2W1","BYFQ60B2W1","BYFQ60B2W1","BYFQ60B2W1"]
["","Barva","","","","Bílá (RAL9010)","Bílá (RAL9010)","Bílá (RAL9010)","Bílá (RAL9010)"]
["","Rozměry","","Výška","mm","55","55","55","55"]
["","","","Šířka","mm","700","700","700","700"]
["","","","Hloubka","mm","700","700","700","700"]
["","Hmotnost","","","kg","2.7","2.7","2.7","2.7"]
["Dekorační panel 4","Model","","","","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1"]
["","Barva","","","","Bílá (RAL9010)","Bílá (RAL9010)","Bílá (RAL9010)","Bílá (RAL9010)"]
["","Rozměry","","Výška","mm","55","55","55","55"]
["","","","Šířka","mm","700","700","700","700"]
["","","","Hloubka","mm","700","700","700","700"]
["","Hmotnost","","","kg","2.7","2.7","2.7","2.7"]
["Řídicí systémy","Infračervené dálkové ovládání","","","","BRC7EB530 (standardní panel), BRC7F530W (bílý panel), BRC7F530S (šedý panel)","BRC7EB530 (standardní panel), BRC7F530W (bílý panel), BRC7F530S (šedý panel)","BRC7EB530 (standardní panel), BRC7F530W (bílý panel), BRC7F530S (šedý panel)","BRC7EB530 (standardní panel), BRC7F530W (bílý panel), BRC7F530S (šedý panel)"]
["","Kabelové dálkové ovládání","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["Standardní příslušenství","Washer for hanger bracket","","","","8","8","8","8"]
["","Thermal insulation tube","","","","2","2","2","2"]
["","Hose band","","","","1","1","1","1"]
["","Drain hose","","","","1","1","1","1"]
["","Installation and operation manual","","","","1","1","1","1"]
["","Screws","","","","4","4","4","4"]
["","Sealing material","","","","4","4","4","4"]
["","Tie-wraps","","","","7","7","7","7"]
["Napájení","Fáze","","","","1~","1~","1~","1~"]
["","Frekvence","","","Hz","50","50","50","50"]
["","Napětí","","","V","220-240","220-240","220-240","220-240"]