{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":6,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFQ-B9V / RXS-F"]
[]
[]
[]
[]
["","","","","FFQ60B9V1B / RXS60F3V1B","FFQ60B9V1B / RXS60F4V1B"]
["Chladicí výkon","Jm.","","kW","5.80 (3)","5.80 (3)"]
["Jmenovitá účinnost","Annual energy consumption","","kWh","1,035","1,035"]
["","EER","","","2.80","2.80"]
["","COP","","","2.81","2.81"]
["","Směrnice o energetických štítcích","Chlazení","","D","D"]
["","","Vytápění","","D","D"]
["Topný výkon","Jm.","","kW","7.00 (4)","7.00 (4)"]
["Poznámky","","","","(1) - Štítek spotřeby: stupnice od A (nejúčinnější) do G (nejméně účinné)","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU"]
["","","","","(2) - Roční spotřeba energie: počítáno podle průměrného používání po dobu 500 provozních hodin za rok při plné zátěži (= jmenovité podmínky)","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení"]
["","","","","(3) - Chlazení: vnitřní teplota 27° CDB, 19° CWB; vnější teplota 35 °CST; ekvivalentní délka potrubí: 7,5 m; rozdíl úrovně: 0m"]
["","","","","(4) - Vytápění: vnitřní teplota 20° CDB; vnější teplota 7° CDB, 6° CWB ekvivalentní délka potrubí chladiva: 7,5 m; rozdíl úrovně: 0m"]
["","","","","(5) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení"]