{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A(9) / RXS-L3"]
[]
[]
[]
[]
["","","","","FHA35AVEB9 / RXS35L3V1B","FHA35AVEB99 / RXS35L3V1B"]
["Chladicí výkon","Jm.","","kW","3.40","3.40"]
["Prostorové chlazení","Roční spotřeba energie","","kWh/rok","","193"]
["","Kapacita","Pnávrh","kW","","3.40"]
["Prostorové vytápění (průměrné klima)","Výkon","Pnávrh","kW","","3.10"]
["","Roční spotřeba energie","","kWh/rok","","981"]
["Jmenovitá účinnost","Roční spotřeba energie","","kWh","459","459"]
["","EER","","","3.70","3.70"]
["","COP","","","4.08","4.08"]
["","Směrnice oenergetických štítcích","Chlazení","","A","A"]
["","","Vytápění","","A","A"]
["Topný výkon","Jm.","","kW","4.00","4.00"]
["Poznámky","","","","(1) - Aplikace „Code du travail“ jsou pro neveřejné budovy (např. kanceláře)","(1) - Jmenovité chladicí výkony vycházejí z těchto podmínek: vnitřní teplota: 27°CDB, 19°CWB, venkovní teplota: 35 °CDB, ekvivalentní délka potrubí s chladivem: 5 m, rozdíl úrovní: 0 m."]
["","","","","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m.","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m."]
["","","","","(3) - Viz samostatný výkres s provozním rozsahem","(3) - Viz samostatný výkres s provozním rozsahem"]
["","","","","(4) - Údaje o elektrickém systému najdete v samostatném výkresu","(4) - Údaje o elektrickém systému najdete v samostatném výkresu"]
["Prostorové chlazení","SEER","","","","6.18"]
["","Třída energetické úspornosti","","","","A++"]
["Prostorové vytápění (průměrné klima)","SCOP/A","","","","4.43"]
["","Třída energetické účinnosti","","","","A+"]