{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RXM-M9"]
[]
[]
[]
[]
["","","","","FHA35AVEB / RXM35M3V1B9","FHA50AVEB / RXM50M3V1B9","FHA60AVEB / RXM60M3V1B9"]
["Chladicí výkon","Jm.","","kW","3.40"]
["Prostorové chlazení","SEER","","","6.24"]
["","Roční spotřeba energie","","kWh/a","191"]
["","Kapacita","Pnávrh","kW","3.40"]
["","Třída energetické úspornosti","","","A++"]
["Prostorové vytápění (průměrné klima)","Výkon","Pnávrh","kW","3.10"]
["","SCOP/A","","","4.43"]
["","Třída energetické účinnosti","","","A+"]
["","Roční spotřeba energie","","kWh/a","979"]
["Jmenovitá účinnost","Roční spotřeba energie","","kWh","456"]
["","EER","","","3.73"]
["","COP","","","4.08"]
["","Směrnice oenergetických štítcích","Chlazení","","A"]
["","","Vytápění","","A"]
["Topný výkon","Jm.","","kW","4.00"]
["Poznámky","","","","(1) - Údaje o elektrickém systému najdete v samostatném výkresu"]
["","","","","(2) - Viz samostatný výkres s provozním rozsahem"]
["","","","","(3) - Jmenovité chladicí výkony vycházejí z těchto podmínek: vnitřní tep.: 27°CDB, 19°CWB, venkovní teplota: 35 °CDB, ekvivalentní délka potrubí s chladivem: 5 m, rozdíl úrovní: 0 m."]
["","","","","(4) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m."]
["Venkovní jednotka","","","","","RXM50M3V1B9","RXM60M3V1B9"]
["Chladicí výkon","Jm.","","kW","","5.00","5.70"]
["Topný výkon","Jm.","","kW","","6.00","7.20"]
["Jmenovitá účinnost","EER","","","","3.21","3.29"]
["","COP","","","","3.35","3.32"]
["","Roční spotřeba energie","","kWh","","780","867"]
["","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích-=-Chlazení","","","B","A"]
["","","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích-=-Vytápění","","","C","C"]
["Prostorové chlazení","Třída energetické úspornosti","","","","A+","A+"]
["","Kapacita","Pnávrh","kW","","5.00","5.70"]
["","SEER","","","","5.92","6.08"]
["","Roční spotřeba energie","","kWh/a","","295","328"]
["Prostorové vytápění (průměrné klima)","Třída energetické účinnosti","","","","A","A"]
["","Výkon","Pnávrh","kW","","4.35","4.71"]
["","SCOP/A","","","","3.86","3.87"]
["","Topný výkon Pdh při -10°","","kW","","3.85","4.08"]
["","Roční spotřeba energie","","kWh/a","","1578","1704"]