{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":6,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RZASG-MY1"]
[]
[]
[]
[]
["","","","","FHA35AVEB / FHA35AVEB / FHA35AVEB / RZASG100M7Y1B","FHA50AVEB / FHA50AVEB / RZASG100M7Y1B"]
["Venkovní jednotka","","","","RZASG100M7Y1B","RZASG100M7Y1B"]
["Chladicí výkon","Jm.","","kW","9.50","9.50"]
["Topný výkon","Jm.","","kW","10.8","10.8"]
["Prostorové chlazení","Třída energetické úspornosti","","","A++","A+"]
["","Kapacita","Pnávrh","kW","9.50","9.50"]
["","SEER","","","7.26","5.79"]
["","Roční spotřeba energie","","kWh/a","458","574"]
["Prostorové vytápění (průměrné klima)","Třída energetické účinnosti","","","A+","A"]
["","Výkon","Pnávrh","kW","6.00","6.00"]
["","SCOP/A","","","4.02","3.92"]
["","Roční spotřeba energie","","kWh/a","2090","2143"]
["Poznámky","","","","(1) - Jmenovité chladicí výkony vycházejí z těchto podmínek: vnitřní tep.: 27°CDB, 19°CWB, venkovní teplota: 35 °CDB, ekvivalentní délka potrubí s chladivem: 5 m, rozdíl úrovní: 0 m.","(1) - Jmenovité chladicí výkony vycházejí z těchto podmínek: vnitřní tep.: 27°CDB, 19°CWB, venkovní teplota: 35 °CDB, ekvivalentní délka potrubí s chladivem: 5 m, rozdíl úrovní: 0 m."]
["","","","","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m.","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m."]