{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":17,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FHA71AVEB / FHA71AVEB / RZQG125L8Y1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQG125L8Y1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQG100L8Y1B","FHA50AVEB / FHA50AVEB / FHA50AVEB / RZQG125L8Y1B","FHA50AVEB / FHA50AVEB / RZQG100L8Y1B","FHA60AVEB / FHA60AVEB / RZQG125L8Y1B","FHA35AVEB / FHA35AVEB / RZQG71L8Y1B","FHA50AVEB / FHA50AVEB / RZQG71L8Y1B","FHA71AVEB / RZQG71L8Y1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQG71L8Y1B","FHA71AVEB / FHA71AVEB / RZQG100L8Y1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQG100L8Y1B","FHA50AVEB / FHA50AVEB / FHA50AVEB / RZQG100L8Y1B"]
["Energetickou účinná řada","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Prostorové chlazení","SEER","","","","","","","","","5.10","5.10","6.86","5.10","5.10","5.10","5.10"]
["","Roční spotřeba energie","","kWh/a","","","","","","","467","467","347","467","652","652","652"]
["","Kapacita","Pnávrh","kW","","","","","","","6.80","6.80","6.80","6.80","9.50","9.50","9.50"]
["","Třída energetické úspornosti","","","","","","","","","A","A","A++","A","A","A","A"]
["Prostorové vytápění (průměrné klima)","Výkon","Pnávrh","kW","","","","","","","6.00","6.00","7.60","6.00","11.30","11.30","11.30"]
["","SCOP/A","","","","","","","","","3.80","3.80","4.32","3.80","3.80","3.80","3.80"]
["","Třída energetické účinnosti","","","","","","","","","A","A","A+","A","A","A","A"]
["","Roční spotřeba energie","","kWh/a","","","","","","","2,211","2,211","2,463","2,211","4,164","4,164","4,164"]
["Poznámky","","","","","","","","","","(1) - Chlazení: vnitřní teplota 27° CDB, 19° CWB; vnější teplota 35 °CST; ekvivalentní délka potrubí: 7,5 m; rozdíl úrovně: 0m","","(1) - Chlazení: vnitřní teplota 27° CDB, 19° CWB; vnější teplota 35 °CST; ekvivalentní délka potrubí: 7,5 m; rozdíl úrovně: 0m"]
["","","","","","","","","","","(2) - Vytápění: vnitřní teplota 20° CDB; vnější teplota 7° CDB, 6° CWB ekvivalentní délka potrubí chladiva: 7,5 m; rozdíl úrovně: 0m","","(2) - Vytápění: vnitřní teplota 20° CDB; vnější teplota 7° CDB, 6° CWB ekvivalentní délka potrubí chladiva: 7,5 m; rozdíl úrovně: 0m"]
["","","","","","","","","","","(3) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","","(3) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU"]
["Chladicí výkon","Jm.","","kW","","","","","","","","","6.80 (1)"]
["Jmenovitá účinnost","Roční spotřeba energie","","kWh","","","","","","","","","890"]
["","EER","","","","","","","","","","","3.82 (3)"]
["","COP","","","","","","","","","","","4.13 (3)"]
["","Směrnice o energetických štítcích","Chlazení","","","","","","","","","","A"]
["","","Vytápění","","","","","","","","","","A"]
["Topný výkon","Jm.","","kW","","","","","","","","","7.50 (2)"]