{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-C / RXS-F"]
[]
[]
[]
[]
["","","","","FHQ60CAVEB / RXS60F4V1B"]
["Chladicí výkon","Jm.","","kW","5.7"]
["Topný výkon","Jm.","","kW","7.2"]
["Jmenovitá účinnost","EER","","","3.26"]
["","COP","","","3.32"]
["","Roční spotřeba energie","","kWh","875"]
["","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích-=-Chlazení","","A"]
["","","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích-=-Vytápění","","C"]
["Prostorové chlazení","Třída energetické úspornosti","","","A"]
["","Kapacita","Pnávrh","kW","7.20"]
["","SEER","","","5.54"]
["","Roční spotřeba energie","","kWh/a","360"]
["Prostorové vytápění (průměrné klima)","Třída energetické účinnosti","","","A"]
["","Výkon","Pnávrh","kW","5.07"]
["","SCOP/A","","","3.50"]
["","Roční spotřeba energie","","kWh/a","2,026.36"]
["Poznámky","","","","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU"]
["","","","","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení"]