{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":7,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-C / RXS-L"]
[]
[]
[]
[]
["","","","","FHQ35CAVEB / RXS35L2V1B","FHQ50CAVEB / RXS50L2V1B","FHQ60CAVEB / RXS60L2V1B"]
["Chladicí výkon","Min.","","kW","1.4","1.7","1.7"]
["","Max.","","kW","4.0","5.3","5.7"]
["","Jm.","","kW","3.40","5.0","5.7"]
["Spoje potrubí","Kapalina","Vnější průměr","mm","6.35","6.35","6.35"]
["","Plyn","Vnější průměr","mm","9.5","12.7","12.7"]
["","Vypouštění","OD","mm","VP20","VP20 (Vnější průměr 26, Vnitřní průměr 20)","VP20 (Vnější průměr 26, Vnitřní průměr 20)"]
["Jmenovitá účinnost","Roční spotřeba energie","","kWh","475","785","875"]
["","EER","","","3.58","3.18","3.26"]
["","COP","","","4.08","3.35","3.32"]
["","Směrnice oenergetických štítcích","Chlazení","","A","B","A"]
["","","Vytápění","","A","C","C"]
["Topný výkon","Jm.","","kW","4.00","6.0","7.20"]
["","Min.","","kW","1.3","1.7","1.7"]
["","Max.","","kW","5.1","6.0","7.2"]
["Poznámky","","","","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU"]
["","","","","(2) - 220 V","(2) - 220 V","(2) - 220 V"]
["","","","","(3) - 230V","(3) - 230V","(3) - 230V"]
["","","","","(4) - 240 V","(4) - 240 V","(4) - 240 V"]
["","","","","(5) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení","(5) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení","(5) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení"]