{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-C / RXS-L3"]
[]
[]
[]
[]
["","","","","FHQ35CAVEB / RXS35L3V1B"]
["Chladicí výkon","Min.","","kW","1.4"]
["","Max.","","kW","4.0"]
["","Jm.","","kW","3.40 (2)"]
["Spoje potrubí","Kapalina","Vnější průměr","mm","6.35"]
["","Plyn","OD","mm","9.5"]
["","Drain","OD","mm","VP20"]
["Jmenovitá účinnost","Roční spotřeba energie","","kWh","475"]
["","EER","","","3.58 (1)"]
["","COP","","","4.08 (1)"]
["","Směrnice oenergetických štítcích","Chlazení","","A"]
["","","Vytápění","","A"]
["Topný výkon","Jm.","","kW","4.00 (2)"]
["","Min.","","kW","1.3"]
["","Max.","","kW","5.1"]
["Poznámky","","","","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU"]
["","","","","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení"]
["","","","","(3) - 220 V"]
["","","","","(4) - 230V"]
["","","","","(5) - 240 V"]